For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Refrigerant-134a System Capacity | 0.35-0.45 kg, 350-450 g | 12.0-16.0 fl oz, 0.77-0.99 lbs
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) | 100 ml | 3.5 fl oz
Refrigerant Oil - Polyalkaline Glycol (PAG) Add When Replacing Condenser | 20-30 ml | 0.7-1.0 fl oz
Refrigerant Oil - Polyalkaline Glycol (PAG) Add When Replacing Receiver/Dryer | 40 ml | 1.5 fl oz