For 1990-2009 cars

### Removal Procedure

1. Remove the headlamps. Refer to Headlamp Replacement in Lighting Systems.
2. Remove the front side marker lamps. Refer to Front Side Marker Lamp Replacement in Lighting Systems.
3. Remove the 7 plastic retainers along the top which secure the front bumper fascia.
4. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
5. Remove the bolt (1) and the plastic retainer (3) which secure the front bumper fascia (2) at each side.
6. Remove the 3 bolts (2) which secure the front bumper fascia (1) along the bottom.
7. Slide forward and remove the front bumper fascia (1) from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the front bumper fascia (1) to the vehicle. Ensure that the front side marker lamps wiring harness is routed into position. Secure the fascia with the 3 bolts (2) along the bottom.

Tighten
Tighten the front bumper fascia bolts to 15 N·m (11 lb ft).

2. Install the bolt (1) and the plastic retainer (3) which secure the front bumper fascia (2) at each side.

Tighten
Tighten the front bumper fascia bolt to 15 N·m (11 lb ft).

3. Lower the vehicle.
4. Install the 7 plastic retainers along the top which secure the front bumper fascia.
5. Install the front side marker lamps. Refer to Front Side Marker Lamp Replacement in Lighting Systems.
6. Install the headlamps. Refer to Headlamp Replacement in Lighting Systems.