For 1990-2009 cars

#### Inflatable Restraint IP Module

Connector Part Information |

• | 09707-02W01-22

• | YEL

Pin | Wire Color | Function
--- | --- | ---
A | YEL | Passenger Frontal Low
B | YEL/RED | Passenger Frontal High

#### Inflatable Restraint Sensing And Diagnostic Module

Connector Part Information |

• | 09706-34KA0-22

• | YEL

Pin | Wire Color | Function
--- | --- | ---
A1 | BLU/RED | Ignition Positive Voltage
A2 | -- | Not Used
A3 | YEL/RED | Passenger Frontal High
A4 | WHT/BLK | Serial Data Line
A5 | -- | Not Used
A6 | GRN/RED | Driver Frontal High
A7 | GRN | Driver Frontal Low
A8 | YEL | Passenger Frontal Low
A9 | BLU | AIR BAG Indicator Lamp Control
A10-A13 | -- | Not Used
A14 | PPL | Communication Input (Not used)
A15 | YEL/BLU | Seat Belt Switch Signal
A16-A17 | -- | Not Used
A18 | BLK | Ground
B1-B8 | -- | Not Used
C1-C8 | -- | Not Used

#### Inflatable Restraint Steering Wheel Module Coil

Connector Part Information |

• | 09707-02W01-22

• | YEL

Pin | Wire Color | Function
--- | --- | ---
A | GRY | Driver Frontal Low
B | WHT | Driver Frontal High