For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Differential Backlash | 0.13 mm-0.18 mm | 0.005 in-0.007 in
Differential Side Bearing Preload (Case Spread) | 0.0508 mm-0.1524 mm | 0.002 in-0.006 in
Differential Side Gear End Play | 12 mm-37 mm | 0.005 in-0.014 in
Differential Side Gear Preload (Maximum) | 2.4 N·m | 21 lb in
Pinion Bearing Preload Starting Torque | 1.2 N·m | 11 lb in
Rear Axle Shaft Length Left Rear Axle Shaft | 683.5 mm | 26.9 in
Rear Axle Shaft Length Right Rear Axle Shaft | 726.5 mm | 28.6 in