For 1990-2009 cars

## Front Seat Adjuster Track Finish Cover Replacement Outer

### Removal Procedure

1. Remove the front seat recliner knob. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .
2. Remove the screw (3) and gently pry the seat outer adjuster finish cover (2) from the seat outer adjuster.

### Installation Procedure

1. Install the seat outer adjuster finish cover (2) to the seat outer adjuster. Secure the cover with the screw (3).
2. Install the front seat recliner knob. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .

## Front Seat Adjuster Track Finish Cover Replacement Inner

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the following components from the seat inner adjuster (2):

• | The 2 screws (3)

• | The seat inner adjuster finish cover (1)

### Installation Procedure

1. Install the seat inner adjuster finish cover (1) to the seat inner adjuster (2). Secure the cover with the 2 screws (3).
2. Install the front seat. Refer to Front Seat Replacement - Bucket .