For 1990-2009 cars

Application | Front Runout | Center Runout | Rear Runout
--- | --- | --- | ---
Metric | English | Metric | English | Metric | English
One-Piece Rear Propeller Shaft (2DR & 4DR - 4WD) | 0.80 mm | 0.031 in | 0.80 mm | 0.031 in | 0.80 mm | 0.031 in
Front Propeller Shaft with Slip Yoke (4DR) | 0.80 mm | 0.031 in | 0.80 mm | 0.031 in | 0.80 mm | 0.031 in
Two-Piece System, Rear Propeller Shaft (4DR -2WD) | 0.80 mm | 0.031 in | 0.80 mm | 0.031 in | 0.80 mm | 0.031 in