For 1990-2009 cars

## Bracket Replacement - Rear Wheel Opening Flare ZR2 Models

### Removal Procedure

1. Remove the rear wheel opening flare. Refer to Bracket Replacement - Rear Wheel Opening Flare .
2. Drill out and remove the 5 rivets (3) that retain the rear wheel opening flare bracket (4).
3. Remove the bracket (4) from the quarter panel (2).

### Installation Procedure

1. Install the rear wheel opening flare bracket (4) to the quarter panel (2). Secure the bracket with 5 rivets (3).
2. Install the rear wheel opening flare. Refer to Bracket Replacement - Rear Wheel Opening Flare .