For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Transmission Oil Pan Bolt | 11 | -- | 96
Vacuum Modulator Assembly Bolt | 52 | 33 | --
Extension Housing to Case Bolt | 31 | 23 | --
Line Pressure Test Plug | 8 | -- | 71
Converter Housing to Cylinder Block Bolt | 34 | 25 | --
Transmission Support to Case Extension Bolt | 44 | 33 | --
Shift Lever to Selector Lever Shaft Bolt | 27 | 20 | --
Detent Cable Retainer to Case Bolt | 9 | -- | 80
Oil Cooler Fittings to Case | 20 | 15 | --
Oil Cooler Fittings to Radiator | 27 | 20 | --
Oil Cooler Hose Clamps to Cooler Lines | 1 | -- | 9
Shifter Assembly to Console Bolt | 9 | -- | 80
Neutral Safety Switch to Bracket Bolt | 2 | -- | 18
Lower Cover to Converter Housing Bolt | 10 | -- | 89
Flexplate to Converter Bolt | 48 | 35 | --
Reinforcement Plate to Case Bolt | 19 | 14 | --
Control Valve Body Assembly to Case Bolt | 19 | 14 | --
Servo Cover to Case Bolt | 24 | 18 | --
Converter Housing To Case Bolt | 33 | 25 | --
Converter Housing to Oil Pump Bolt | 19 | 14 | --
Manual Shaft Lever Locknut | 12 | 9 | --
Governor Body to Governor Hub Bolt | 8 | -- | 71
Servo Adjusting Bolt Locknut | 18 | 14 | --
Governor Pressure Switch | 10 | -- | 89
Solenoid | 19 | 14 | --
Oil Filter Bolt | 19 | 14 | --

Fastener Tightening | Specification
--- | ---
Metric | English
Cooler Pipe Clamp Bolt | 23 N·m | 17 lb ft
Cooler Pipe Flare Nuts | 25 N·m | 18 lb ft
Engine Rear Mounting Bolts (Four-Wheel Drive Models) | 50 N·m | 37 lb ft
Engine Rear Mounting Member Bolts (Four Wheel Drive Models) | 50 N·m | 37 lb ft
Exhaust Pipe Bracket Bolt and Nuts (3L30, 3-Speed) | 23 N·m | 17 lb ft
Extension Housing Bolts (3L30, 3-Speed) | 31 N·m | 23 lb ft
Fluid Cooler Hose Clamps | 1.5 N·m | 12 lb in
Fluid Filler Tube Bracket Bolt | 23 N·m | 17 lb ft
Fluid Filter Screen Bolts (3L30, 3-Speed) | 19 N·m | 14 lb ft
Fluid Pressure Switch | 10 N·m | 89 lb in
Flywheel Inspection Cover Bolts | 10 N·m | 89 lb in
Flywheel to Torque Converter Bolts (3L30, 3-Speed) | 55 N·m | 40 lb ft
Front Propeller Shaft Bolts and Nuts (Four-Wheel Drive Models) | 50 N·m | 37 lb ft
Front Skid Plate Bolts | 54 N·m | 40 lb ft
Governor Assembly Bolts (3L30, 3-Speed) | 9 N·m | 80 lb in
Interlock Cable Nut | 13 N·m | 115 lb in
Lower Transmission Retaining Nuts | 85 N·m | 62 lb ft
Manual Select Lever Nut | 19 N·m | 14 lb ft
Manual Selector Bolts | 18 N·m | 13 lb ft
Park/Neutral Position Switch Bolt | 21 N·m | 15 lb ft
Rear Propeller Shaft Bolts and Nuts | 50 N·m | 37 lb ft
Rear Propeller Shaft Bolts and Nuts | 50 N·m | 37 lb ft
Rear Transmission Crossmember Bolts (Two-Wheel Drive Models) | 60 N·m | 44 lb ft
Rear Transmission Mount Bolts (Two-Wheel Drive Models) | 60 N·m | 44 lb ft
Reinforcement Plate Bolts (3L30, 3-Speed) | 19 N·m | 14 lb ft
Servo Piston Cover Bolts (3L30, 3-Speed) | 25 N·m | 18 lb ft
Shift Lock Solenoid Retaining Bolt | 10 N·m | 89 lb in
Shift Select Cable Locknut | 7 N·m | 62 lb in
Speedometer Guide Bracket Bolt | 9 N·m | 80 lb in
Starter Motor Bolts | 30 N·m | 22 lb ft
Stoplamp Switch Adjustment Nut | 15 N·m | 11 lb ft
TCC Solenoid Retaining Bolts (3L30, 3-Speed) | 19 N·m | 14 lb ft
Torque Stopper Bushing Bolts (Four Wheel Drive Models) | 50 N·m | 37 lb ft
Transfer Adapter Case Bolts | 31 N·m | 23 lb ft
Transfer Plate-to-Valve Body Bolts | 9 N·m | 80 lb in
Transmission Fluid Pan Bolts (3L30, 3-Speed) | 13 N·m | 115 lb in
Transmission Range Switch Bolt to | 5 N·m | 44 lb in
Transmission Range Switch Set Nut to | 5 N·m | 44 lb in
TV Cable Retaining Bracket Bolt (3L30, 3-Speed) | 10 N·m | 89 lb in
Upper Transmission Retaining Bolts | 85 N·m | 62 lb ft
Vacuum Modulator (3L30, 3-Speed) | 52 N·m | 38 lb ft
Valve Body Bolts (3L30, 3-Speed) | 19 N·m | 14 lb ft