For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Differential Carrier Nuts | 55 N·m | 41 lb ft
Differential Side Bearing Cap Bolts | 100 N·m | 72 lb ft
Jam Nut | 2 N·m | 18 lb in
Load Sensing Spring Bracket Bolts | 18-25 N·m | 13.5-20.0 lb ft
Lower Shock Absorber Through Bolts and Nuts | 85 N·m | 63 lb ft
Rear Axle Housing Drain Plug | 25 N·m | 18 lb ft
Rear Axle Housing Oil Level/Filler Plug | 43 N·m | 32 lb ft
Rear Axle Shaft Retaining Nuts | 23 N·m | 17 lb ft
Rear Control Arm Ball Joint Boss Bolts | 50 N·m | 37 lb ft
Rear Control Arm Through Bolts and Nuts | 90 N·m | 66 lb ft
Rear Propeller Shaft Bolts and Nuts | 50 N·m | 37 lb ft
Rear Trailing Rod Through Bolts and Nuts | 90 N·m | 66 lb ft
Rear Wheel Speed Sensor Bolt | 23 N·m | 17 lb ft
Rear Wheel Speed Sensor Cover Bolts | 15 N·m | 11 lb ft
Ring Gear Bolts | 90 N·m | 65 lb ft
Side Bearing Lock Plate Bolts | 33 N·m | 25 lb ft