For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Clutch pedal effort and clutch pedal travel are normal.
1 | Inspect the clutch master cylinder fluid level. Is the clutch hydraulic system fluid level OK? | Go to Step 4 | Go to Step 2
2 | Inspect the clutch master cylinder and clutch actuator cylinder. Is the clutch master cylinder and clutch actuator cylinder assemblies working properly? | Go to Step 4 | Go to Step 3
3 | Replace the required clutch hydraulic system components. Refer to Clutch Master Cylinder Replacement . Is gear selection operation normal? | System OK | Go to Step 4
4 | Replace the required clutch components Does the clutch work properly? | System OK | --