For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Antilock Brake System (ABS) Resister | RH I/P, behind I/P Compartment taped to Main Harness | -- | Antilock Brake System Connector End Views in Antilock Brakes
Daytime running Lamps (DRL) Control Module | Behind I/P, left of Steering Column on Powertrain Control Module (PCM) mounting bracket | -- | --
Diode No. 2 | Main Harness, behind I/P Compartment taped to harness | -- | --
Electronic Brake Control Module (EBCM) (with ABS) | Under LH I/P, right of Steering Column | Antilock Brake System Component Views in Antilock Brakes | --
Electronic Brake Control Module (EBCM) (with ABS) C1 (32 Cavities) | Main Harness to EBCM, behind I/P right of Steering Column | -- | Antilock Brake System Connector End Views in Antilock Brakes
Electronic Brake Control Module (EBCM) (with ABS) C2 (2 Cavities) | Main Harness to EBCM, behind I/P right of Steering Column | -- | Antilock Brake System Connector End Views in Antilock Brakes
Fuse Block 1 | RH Engine Compartment, front of Battery | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views in Wiring Systems | --
Ignition Switch | On Steering Column | Power and Grounding Component Views in Wiring Systems | --
Instrument Panel Cluster Assembly | LH I/P | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Instrument Panel Cluster Assembly C1 (16 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Instrument Panel Cluster Assembly C3 (13 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Parking Brake Switch | In Center Console, left of Parking Brake Lever | -- | --
C200 (22 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views in Wiring Systems | --
C211 (16 Cavities) | I/P Harness to Floor Harness, LH I/P, near A-Pillar | Harness Routing Views in Wiring Systems | --
C301 (6 Cavities) (2-Door) | Floor Harness to Sub-Floor Harness, behind LH Rear Passenger Compartment Trim Panel | -- | --
G101 | On Bulkhead behind Distributor | Harness Routing Views in Wiring Systems | --
G102 | RH Rear of Engine near Distributor | Harness Routing Views in Wiring Systems | --
G105 (with ABS) | RH Inner Fender, near Battery | Harness Routing Views in Wiring Systems | --
G200 | Behind LH I/P, above Fuse Block 2 | Harness Routing Views in Wiring Systems | --
G202 | Behind Center I/P on Bulkhead | -- | --
P200 | LH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views in Wiring Systems | --
P201 | RH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views in Wiring Systems | --
P300 (2-Door) | LH A-Pillar, under I/P, behind LH Kick Panel | Harness Routing Views in Wiring Systems | --
S106 | Main Harness, approximately 10 cm from Noise Suppressor Filter connector breakout | -- | --
S204 | I/P Harness, approximately at C211 breakout | Harness Routing Views in Wiring Systems | --
S208 | Main Harness, approximately 18 cm from Ignition Switch connector breakout | Harness Routing Views in Wiring Systems | --
S210 | Main Harness, approximately 12 cm from Stoplamp Switch connector breakout | -- | --
S211 (with ABS) | Main Harness, approximately 9 cm from Electronic Brake Control Module (EBCM) connector C2 breakout | Harness Routing Views in Wiring Systems | --
S214 | Main Harness, approximately 10 cm from C216 breakout | Harness Routing Views in Wiring Systems | --
S222 | Main Harness, approximately 10 cm from Blower Speed Selector Switch connector breakout | Harness Routing Views in Wiring Systems | --
S227 | Main Harness, approximately 8 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S229 | Main Harness, approximately 7 cm from Ignition Switch connector breakout | Harness Routing Views in Wiring Systems | --
S230 | Main Harness, approximately 5 cm from G300 breakout | Harness Routing Views in Wiring Systems | --
S262 | Main Harness, approximately 8 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S270 (with ABS) | Main Harness, approximately 12 cm from Electronic Brake Control Module (EBCM) connector C2 breakout | Harness Routing Views in Wiring Systems | --
S271 (with ABS) | Main Harness, approximately 2 cm from C212 breakout | Harness Routing Views in Wiring Systems | --
S272 | Main Harness, approximately 11 cm from G200 breakout | Harness Routing Views in Wiring Systems | --
S281 | Main Harness, approximately 3 cm from C203 breakout | -- | --