For 1990-2009 cars

## Front Side Door Sill Trim Plate Replacement 2 Door

### Removal Procedure

Remove the following components from the vehicle:

1. The 4 plastic retainers (2)
2. The front side door sill trim plate (1)

### Installation Procedure

Install the front side door sill trim plate (1) to the vehicle. Secure the trim plate with the 4 plastic retainers (2).

## Front Side Door Sill Trim Plate Replacement 4 Door

### Removal Procedure

Remove the following components from the vehicle:

1. The 3 plastic retainers (2)
2. The front side door sill trim plate (1)

### Installation Procedure

Install the front side door sill trim plate (1) to the vehicle. Secure the trim plate with the 3 plastic retainers (2).