For 1990-2009 cars

## Body Hinge Pillar Trim Panel Replacement Left

### Removal Procedure

1. Remove the front floor foot rest (1). Refer to Foot Rest Replacement .
2. Remove the following components from the vehicle:

2.1. | The 2 plastic retainers (5)

2.2. | The body hinge pillar trim panel (4)

### Installation Procedure

1. Install the body hinge pillar trim panel (4) to the vehicle. Secure the trim panel with the 2 plastic retainers (5).
2. Install the front floor foot rest (1). Refer to Foot Rest Replacement .

## Body Hinge Pillar Trim Panel Replacement Right

### Removal Procedure

Remove the following components from the vehicle:

1. The 2 plastic retainers
2. The body hinge pillar trim panel

### Installation Procedure

Install the body hinge pillar trim panel to the vehicle. Secure the trim panel with the 2 plastic retainers.