For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1-2 Shift Solenoid (1-2 SS) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | --
2-3 Shift Solenoid (2-3 SS) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | --
A/C Compressor Clutch Coil | Part of the A/C compressor, right side of engine at the end of the crankshaft, near the crankshaft position sensor (24x) | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
A/C Refrigerant Pressure Sensor | Left side of the engine compartment, below the accumulator, below the air cleaner assembly | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Air Inflator Switch | Behind the left rear wheelhouse | Automatic Level Control Component Views in Automatic Level Control | Automatic Level Control Connector End Views in Automatic Level Control
Air Injection Bleed Valve | Left rear of engine, above valve cover | -- | Engine Controls Connector End Views in Engine Controls-3.4L
AIR Pump Relay | Forward lamp harness, right side of the engine compartment, rearward of the Horn | Power and Grounding Component Views | Power and Grounding Connector End Views
Ambient Air Temperature Sensor | In front of the radiator, right side | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Ashtray Lamp | Center of IP, mounted to the back of the ashtray | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Auto Level Control (ALC) Air Compressor | Under the vehicle, behind the left rear wheelhouse | Automatic Level Control Component Views in Automatic Level Control | Automatic Level Control Connector End Views in Automatic Level Control
Auto Level Control (ALC) Air Inflator Relay | In the vehicle, behind the left rear wheelhouse | Automatic Level Control Component Views in Automatic Level Control | Automatic Level Control Connector End Views in Automatic Level Control
Auto Level Control (ALC) Air Inflator Solenoid Valve | Behind the left rear wheelhouse | Automatic Level Control Component Views in Automatic Level Control | Automatic Level Control Connector End Views in Automatic Level Control
Auto Level Control (ALC) Sensor | Mounted to the rear crossmember above the rear axle | Automatic Level Control Component Views in Automatic Level Control | Automatic Level Control Connector End Views in Automatic Level Control
Automatic Transaxle Fluid Temperature (TFT) Sensor | Inside the automatic transaxle | -- | Shift Lock Control Connector End Views in Automatic Transaxle-4T65-E
Automatic Transmission Shift Lock Solenoid | Inside the steering column near the ignition switch | -- | Shift Lock Control Connector End Views in Automatic Transaxle-4T65-E
Auxiliary Blower Motor | Part of the auxiliary heater-A/C module, behind the left rear wheelhouse | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Blower Motor Resistor | Part of the auxiliary heater-A/C module, rear of the auxiliary blower motor | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Heater-A/C Control (Auxiliary Blower Switch) (4 Door) | Part of the left rear armrest | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Heater-A/C Control (Temperature Control) (4 Door) | Part of the left rear armrest | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Heater-A/C Control (Auxiliary Blower Switch) (5 Door) | Part of the rear roof console, behind the driver seat | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Heater-A/C Control (Temperature Control) (5 Door) | Part of the rear roof console, behind the driver seat | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Temperature Valve Actuator | Part of the auxiliary heater-A/C module, below the auxiliary blower motor | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Auxiliary Video Module (AVM) | Overhead console, left side of video screen | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Backup Lamps | Part of the taillamps | -- | --
Backup Lamp Relay | Right side of steering column, behind IP | -- | Lighting Systems Connector End Views in Lighting Systems
Bank 1 Knock Sensor (KS) | Front of the engine, above the starter | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Battery | Engine compartment, behind the right headlamp | -- | --
Blower Motor | Part of the heater-A/C module, behind the right side of the IP compartment | HVAC Component Views in HVAC Systems-Manual | --
Blower Motor Resistor | Part of the heater-A/C module, behind the right side of the IP compartment, in front of the blower motor | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Brake Fluid Level Indicator Sensor | Right side of the brake fluid reservoir | Hydraulic Brake Component Views in Hydraulic Brakes | Hydraulic Brake Connector End Views in Hydraulic Brakes
Brake Modulator | Left side of the engine compartment, mounted to the brake master cylinder | Antilock Brake System Component Views in Antilock Brake System | --
Camshaft Position (CMP) Sensor | Engine compartment, right side of the engine, above the A/C compressor clutch | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Cargo Lamp | Above the liftgate, on the roof headliner | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Center High Mounted Stop Lamp (CHMSL) | Center, top of liftgate | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Cigar Lighter | Center IP, right side of the ashtray | Power and Grounding Component Views | Power and Grounding Connector End Views
Cool Fan 1 Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Cool Fan 2 Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Cool Fan Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Crank Relay | Right side of Engine Compartment on the radiator support, inboard of the underhood accessory wiring junction block | Power and Grounding Component Views | Power and Grounding Connector End Views
Crankshaft Position (CKP) Sensor (7X) | Lower rear of the engine | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Crankshaft Position (CKP) Sensor (24X) | Right side of the engine, at the end of the crankshaft, behind the harmonic balancer | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Cruise Control Module | Engine compartment, near the left strut tower | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Release Switch | Mounted to the brake pedal support | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Switch | Part of the turn signal switch, on the turn signal lever | Theft Deterrent System Component Views in Theft Deterrent | Cruise Control Connector End Views in Cruise Control
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Daytime Running Lamp (DRL) Ambient Light Sensor | Center of IP, secured to the upper trim pad, near the windshield defrost vent | Theft Deterrent System Component Views in Theft Deterrent | Lighting Systems Connector End Views in Lighting Systems
Daytime Running Lamps (DRL) Control Module | Right of the steering column, behind the IP | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Dome Lamp | Center of the roof headliner | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Door Lock Switch Plate (Door Mounted, Striker) | Mounted to the lower, front end of the rear side door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Door Lock Switch Plate (Pillar Mounted, Striker) | Mounted to the lower, rear side of the B-pillar | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Driver Information Display | In the roof console | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Driver Seat Belt Pretensioner | -- | -- | --
Driver Seat Belt Switch | Inside the right half of the driver seat belt | -- | Seat Belt Connector End Views in Seat Belts
Electric Air Inlet Actuator | Right side of the IP, above the blower motor, near the relay center, and the BCM | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Electric Slave Actuator | Left side of the heater-A/C module, left of the radio above the knee bolster | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Electronic Brake Control Module (EBCM) | Lower left side of the engine compartment | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Electronic Brake Control Relay | Part of the EBCM | -- | --
Engine Coolant Fan Motor 1 (RH) | Mounted to the rear left side of the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Fan Motor 2 (LH) | Mounted to the rear right side of the radiator | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Level Indicator Module | Mounted to the rear right side of the radiator, below the radiator cap | Cooling System Component Views in Engine Cooling | Cooling System Connector End Views in Engine Cooling
Engine Coolant Temperature (ECT) Sensor | Left side top of the engine | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Engine Oil Level Indicator Switch | Center of the engine oil pan | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Engine Oil Pressure Indicator Switch | Front of the engine, above the starter | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Evaporative Emissions (EVAP) Canister Purge Solenoid Valve | Top rear of the engine, below the ignition control module | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Evaporative Emissions (EVAP) Canister Vent Solenoid Valve | Below the center of the vehicle, forward of the fuel tank | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Exhaust Gas Recirculation (EGR) Valve | Upper left side of the engine | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Fog Lamps | On the front of the vehicle | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Front Door Lock | Inside, rear end of the front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Door Lock (Actuator) | Part of the front door lock | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Door Lock (Ajar Indicator Switch) | Part of the front door lock | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Door Lock Cylinder Switch | Inside the front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Door Lock Switch | In the front door armrest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Door Speakers | Inside the front door | -- | Entertainment Connector End Views in Entertainment
Front Electric Accessory Plug Housing | Center of the IP, left of the ashtray | Power and Grounding Component Views | Power and Grounding Connector End Views
Front Park/Turn Lamps | In front of the vehicle, next to the headlamps | Lighting Systems Component Views in Lighting Systems | --
Front Roof Rail Reading Lamps | On both sides of the headliner between the B and C-pillars | Lighting Systems Component Views in Lighting Systems | --
Front Side Marker Lamps | Front of the vehicle, on both sides | Lighting Systems Component Views in Lighting Systems | --
Front Window Regulator Motor | Inside the front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Front Window Switch | In the armrest of the front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Fuel Injectors | Top of the engine at each cylinder intake port | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Fuel Level Sender | Mounted inside the fuel tank | -- | --
Fuel Pump Motor | Mounted inside the fuel tank | -- | --
Fuel Pump Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Fuel Tank | Below the left side, middle of the vehicle | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Fusible Link A | Bolted to the starter solenoid | -- | --
Fusible Link C | Bolted to the starter solenoid | -- | --
Fusible Link K | Bolted to the starter solenoid | -- | --
Fusible Link Z | Bolted to the starter solenoid | -- | --
Generator | Top rear right side of the engine | Engine Electrical Component Views in Engine Electrical | Engine Electrical Connector End Views in Engine Electrical
Hazard Lamp Flasher (Export) | Below the IP, above the base of the steering column, left side of the steering column | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Hazard Lamp/Turn Signal Flasher | Below the IP, above the base of the steering column, left side of the steering column | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Headlamps | Front side of the vehicle | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Headlamp Dimmer Switch | Part of the turn signal switch, mounted to the steering column | -- | Lighting Systems Connector End Views in Lighting Systems
Headlamp and IP Lamp Dimmer Switch | Left of the instrument cluster | Lighting Systems Component Views in Lighting Systems | --
Headlamp Position Lamp (Export) | Front of the vehicle | -- | --
Heated Oxygen Sensor 1 (HO2S 1) | Rear of the engine, in the exhaust manifold | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Heated Oxygen Sensor 2 (HO2S 2) | In the exhaust system, behind the catalytic converter | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Heated Seat Module | Under the seat frame at rear of cushion | Power Seat Component Views in Seats | Power Seat Connector End Views in Seats
Heated Seat Switch | Part of the rear window wiper/washer and multi-function switch | Power Seat Component Views in Seats | Power Seat Connector End Views in Seats
Heater-A/C Control | Center of the IP, below the radio | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Heater-A/C Control (Blower Motor Switch) | Part of the heater-A/C control | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Heater-A/C Control (Compressor and Air Delivery Control) | Part of the heater-A/C control | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Heater-A/C Control (Rear Window Defogger Switch) | Part of the heater-A/C control | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Horn Switch | Behind the inflatable restraint steering wheel module | SIR Component Views in SIR | --
Idle Air Control (IAC) Valve | Top of the engine, front of the throttle assembly | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Ignition Control Module (ICM) | Top center rear of the engine | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Ignition Key Alarm Switch | Part of the steering column | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Ignition Switch | Part of the steering column | -- | --
Inflatable Restraint Front Side Impact Module, Left | Left side of the driver seat back cover | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Front Side Impact Module, Right | Right side of the passenger seat back cover | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint IP Module | Right side of the IP top of the dash, above the IP compartment | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Below the right front seat | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Side Impact Sensor, Left | Inside the base of the left B-pillar, above the seat side belt retractor | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Side Impact Sensor, Right | Inside the base of the right B-pillar, above the seat side belt retractor | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Steering Wheel Module | Center of the steering wheel, includes the horn switches | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Steering Wheel Module Coil | Center of the steering wheel, behind the inflatable restraint steering wheel module | SIR Component Views in SIR | SIR Connector End Views in SIR
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Intake Air Temperature (IAT) Sensor | Left of engine compartment, on the air intake duct, near the throttle body | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Interface Module (IM) | Inside overhead console, left corner | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Interior Lamp and Multi-function Switch | Center in front of the roof headliner | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Interior Lamp and Multi-function Switch (Interior Lamps Override Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Interior Lamp and Multi-function Switch (Power Sliding Door On/Off Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views in Lighting Systems | Power Door Systems Connector End Views in Doors
Interior Lamp and Multi-function Switch (Power Sliding Door Open/Close Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views in Lighting Systems | Power Door Systems Connector End Views in Doors
Interior Lamp and Multi-function Switch (Rear Quarter Window Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views in Lighting Systems | Power Door Systems Connector End Views in Doors
IP Compartment Lamp Switch | Inside of the IP compartment, part of the IP compartment lamp | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Left Front Brake Solenoid Valve | Left side of the engine compartment, part of the brake modulator, mounted to the brake master cylinder | Antilock Brake System Component Views in Antilock Brake System | --
Left Front Wheel Speed Sensor | Part of the left front hub assembly | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Left Horn | Front left side of the vehicle, mounted to the left side of the front lower crossmember | Horn Component Views in Horns | Horn Connector End Views in Horns
Left Instrument Panel (IP) Courtesy Lamp | Below left side of the IP, near the park brake | -- | Lighting Systems Connector End Views in Lighting Systems
Left Rear Turn Lamp | Part of the left taillamp | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Left Rear Wheel Speed Sensor | Part of the left rear hub assembly | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
License Lamps | Rear of the vehicle, above the license plate | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Liftgate Door Lock | Inside the liftgate, below the license plate | Body Rear End Component Views in Body Rear End | Body Rear End Connector End Views in Body Rear End
Liftgate Door Lock (Actuator) | Part of the liftgate door lock | Body Rear End Component Views in Body Rear End | Body Rear End Connector End Views in Body Rear End
Liftgate Door Lock (Ajar Indicator Switch) | Part of the liftgate door lock | Body Rear End Component Views in Body Rear End | Body Rear End Connector End Views in Body Rear End
Liftgate Door Lock Cylinder Switch | Inside the liftgate, above the license lamps | Body Rear End Component Views in Body Rear End | Body Rear End Connector End Views in Body Rear End
Manifold Absolute Pressure (MAP) Sensor | Right top of the engine | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Mass Air Flow (MAF) Sensor | Left front of the engine compartment, in the air cleaner duct | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Outside Rearview Mirror | On the outside of the front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Outside Rearview Mirror (Heated Defogger) | In the outside rearview mirror | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Outside Rearview Mirror (Mirror Motor Pack) | In the outside rearview mirror | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Outside Rearview Mirror Remote Control Switch | Mounted to the top front left front door armrest panel | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Park Brake Indicator Switch | Lower left A-pillar, part of the park brake assembly | Hydraulic Brake Component Views in Hydraulic Brakes | Hydraulic Brake Connector End Views in Hydraulic Brakes
Passenger Seat Adjuster Motor Assembly | Under the right front seat | -- | --
Passenger Seat Adjuster Switch | Mounted to the side of the base of the right front seat | -- | --
Passenger Seat Belt Pretensioner | -- | -- | --
PASS-Key® III Module | In the steering column, at the ignition switch | -- | Theft Deterrent System Connector End Views in Theft Deterrent
Power Sliding Door Detent Switch | Inside the right rear door, mounted to the rear of the door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Power Sliding Door Open/Close Switch (RH B-Pillar) | Middle of the right B-pillar | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Power Sliding Door Unlatch Actuator | In the right power sliding door at the front of the door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls-3.4L | Powertrain Control Module Connector End Views in Engine Controls-3.4L
Radio | Center of the IP console | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Radio Control Switches | Left and right sides of the inflatable restraint steering wheel module | Entertainment Component Views in Entertainment | --
Radio Liftgate Speakers | On both sides of the liftgate | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Radio Rear Seat Audio Control (4 Door) | Part of the left rear armrest | HVAC Component Views in HVAC Systems-Manual | Entertainment Connector End Views in Entertainment
Radio Rear Seat Audio Control (5 Door) | Part of the rear roof console, above the driver seat | HVAC Component Views in HVAC Systems-Manual | Entertainment Connector End Views in Entertainment
Radio Rear Seat Audio Control (WU3) | Part of the rear roof console, above the right passenger seat | HVAC Component Views in HVAC Systems-Manual | Entertainment Connector End Views in Entertainment
Rear Door Lock (Actuator) | In the rear side door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Rear Electric Accessory Plug Housing | Inside the vehicle, behind the left rear wheelhouse | -- | Power and Grounding Connector End Views
Rear Fog Lamp Module (Export) | Below left side of steering column | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Rear Fog Lamp Relay | Part of the relay center, right side of the IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | -- | --
Rear Fog Lamps | On the rear of the vehicle | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Rear Quarter Window Actuator | Rear part of the rear quarter window, on the D-pillar | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Rear Roof Rail Reading Lamps | On both sides of the roof headliner, behind the left C-pillar and the left D-pillars | Lighting Systems Component Views in Lighting Systems | --
Rear Side Door Actuator Control Module | Right quarter panel, above the wheelhouse | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Rear Side Door Actuator Motor | Right quarter panel, above the wheelhouse | Power Door Systems Component Views in Doors | --
Rear Side Door Actuator Motor (Optical Sensor) | Part of the rear side door actuator motor | Power Door Systems Component Views in Doors | --
Rear Sliding Door Alarm | Attached to the rear side door actuator motor | Power Door Systems Component Views in Doors | --
Rear Window Defogger Grid | Rear liftgate window | Stationary Windows Component Views in Stationary Windows | Stationary Windows Connector End Views in Stationary Windows
Rear Window Washer Pump | Engine compartment, mounted to the rear washer solvent container | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Rear Window Wiper Motor | Center of the liftgate | -- | Wiper/Washer Connector End Views in Wipers/Washer Systems
Rear Window Wiper/Washer and Multi-function Switch | Center of the IP, below the radio | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Rear Window Wiper/Washer and Multi-function Switch (Auxiliary Blower Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views in Wipers/Washer Systems | HVAC Connector End Views in HVAC Systems-Manual
Rear Window Wiper/Washer and Multi-function Switch (Fog Lamp/TCC Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views in Wipers/Washer Systems | Lighting Systems Connector End Views in Lighting Systems
Rear Window Wiper/Washer and Multi-function Switch (Heated Seat Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views in Wipers/Washer Systems | --
Rear Window Wiper/Washer and Multi-function Switch (Rear Window Wiper/Washer Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Power and Grounding Component Views | Power and Grounding Connector End Views
Remote Battery Stud | Engine compartment, connected to the underhood accessory wiring junction block, above the battery | Harness Routing Views | --
Remote Control Door Lock Receiver (RCDLR) | Behind the center of the IP, underside of the IP trim, near the windshield defrost vent | Keyless Entry Component Views in Keyless Entry | Keyless Entry Connector End Views in Keyless Entry
Retained Accessory Power Relay | In the relay center | Power and Grounding Component Views | Power and Grounding Connector End Views
Right Front Brake Solenoid Valve | Left side of the engine compartment, part of the brake modulator, mounted to the brake master cylinder | Antilock Brake System Component Views in Antilock Brake System | --
Right Front Wheel Speed Sensor | Part of the right front hub assembly | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Right Horn | Front right side of the vehicle, mounted to the right side of the front lower crossmember | Horn Component Views in Horns | Horn Connector End Views in Horns
Right IP Courtesy Lamp | Below the right side of the IP | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Right Rear Turn Lamp | Part of the right taillamp | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Right Rear Wheel Speed Sensor | Part of the right rear hub assembly | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Right Sunshade Lighted Vanity Mirror | Part of the right sunshade | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Right Taillamp | Rear of the vehicle, right side | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Right Tail/Stop Lamp | Rear of the vehicle, inside the right taillamp | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Seat Adjuster Motor Assembly | Under the front seat | Power Seat Component Views in Seats | Power Seat Connector End Views in Seats
Seat Adjuster Switch | Mounted to the side of the base of the seat | Power Seat Component Views in Seats | Power Seat Connector End Views in Seats
Seat Belt Switch | Inside the right half of the driver seat belt | Seat Belt Component Views in Seat Belts | Seat Belt Connector End Views in Seat Belts
Second Seat Audio (SSA) Control | Overhead console, right side of video screen | HVAC Component Views in HVAC Systems-Manual | Entertainment Connector End Views in Entertainment
Secondary Air Injection Pump | Mounted in lower portion of the drivers front fender | -- | Engine Controls Connector End Views in Engine Controls-3.4L
Security Indicator Lamp | Center of the IP, mounted to the trim plate, near the windshield defrost vent | Theft Deterrent System Component Views in Theft Deterrent | --
Sliding Door Jamb Switch | Mounted to the rear opening of the rear side door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Starter Motor | Lower front of the engine | -- | --
Starter Solenoid | Lower front of the engine, part of the starter motor assembly | -- | --
Stop Lamp Switch | Mounted to the brake pedal support | Cruise Control Component Views in Cruise Control | Lighting Systems Connector End Views in Lighting Systems
Sunshade Lighted Vanity Mirrors | Part of both sunshades | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Taillamp | Rear of the vehicle, on both sides | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Tail/Stop Lamps | Rear of the vehicle, inside both taillamps | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Tape Retract Module (TRM) | Underneath left side instrument panel, near left side of the Data Link Connector (DLC), taped to the VCP harness | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
TCC Brake Switch | Mounted to the brake pedal support, connector 2 of the stop lamp switch | -- | Automatic Transmission Related Connector End Views in Automatic Transaxle-4T65-E
Theft Deterrent Relay | Part of the relay center, right side of the IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control System | --
Theft Deterrent Shock Sensor | Below the left side IP, right of the steering column | Theft Deterrent System Component Views in Theft Deterrent | Theft Deterrent System Connector End Views in Theft Deterrent
Third Seat Audio (TSA) Control | Right quarter trim panel, next to the third row right seat | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Throttle Position (TP) Sensor | Top of the engine, on the throttle assembly | Engine Controls Component Views in Engine Controls-3.4L | Engine Controls Connector End Views in Engine Controls-3.4L
Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | --
Trailer Wiring Harness | Under the left right side of the vehicle, near the left rear wheelhouse | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | Automatic Transmission Related Connector End Views in Automatic Transaxle-4T65-E
Turn Signal Lever (Cruise Control Switch) | Left side of the steering column, part of the turn signal switch | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Turn Signal and Headlamp Dimmer Switch and Windshield Wiper and Windshield Washer Switch | Inside the steering column | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
Vehicle Speed Sensor (VSS) | Lower right rear of the engine compartment, mounted to the right side of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | Automatic Transmission Related Connector End Views in Automatic Transaxle-4T65-E
Video Cassette Player (VCP) | Front floor console | Entertainment Component Views in Entertainment | --
Video Screen-Liquid Crystal Display (LCD) | In the center of the overhead console | HVAC Component Views in HVAC Systems-Manual | --
Windshield Antenna | Within the windshield | -- | --
Windshield Header Courtesy/Reading Lamps | Part of the roof console | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Windshield Wiper Motor | Top right rear of the engine compartment | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Windshield Washer Pump | Engine compartment, mounted to the front washer solvent container | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Windshield Wiper/Washer Switch | Part of the turn signal switch, on the steering column | Lighting Systems Component Views in Lighting Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views > | Inline Harness Connector End Views
C102 (16 cavities) | Engine wiring harness to the fuel injector wiring harness, top of the engine, near the generator next to C108 | -- | Inline Harness Connector End Views
C105 (4 cavities) | Engine wiring harness to the engine coolant fan wiring harness, behind the engine coolant fan 1 (left) | -- | Inline Harness Connector End Views
C111 (14 cavities) | Engine wiring harness to the automatic transaxle wiring harness, lower left side of the engine compartment, front of the automatic transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle-4T65-E | Automatic Transmission Inline Harness Connector End View in Automatic Transaxle-4T65-E
C120 (3 cavities) | IP wiring harness to the forward lamp wiring harness, between the battery and the windshield fluid reservoir | Harness Routing Views | Inline Harness Connector End Views
C171 (2 cavities) | IP wiring harness to the left wheel speed sensor wiring harness, below the air cleaner assembly, mounted to the left inner fender | Harness Routing Views | Inline Harness Connector End Views
C172 (2 cavities) | IP wiring harness to the right wheel speed sensor wiring harness, below the windshield fluid reservoir | Harness Routing Views | Inline Harness Connector End Views
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C205 (4 cavities) | IP wiring harness to the steering wheel radio control wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views | Inline Harness Connector End Views
C215 (2 cavities) | Inflatable restraint wiring harness to the inflatable restraint steering wheel module wiring harness, mounted to the left side of the steering column near base | Harness Routing Views | Inline Harness Connector End Views
C216 (2 cavities) | Inflatable restraint wiring harness to the inflatable restraint IP module wiring harness, near the front right side of the IP compartment | Harness Routing Views | Inline Harness Connector End Views
C217(8 cavities) | Video Entertainment harness to the video cassette player (VCP) jumper harness behind the VCP | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
C290 (1 cavity) | Antenna coaxial cable wiring harness to the antenna coaxial cable wiring harness, behind the IP compartment | -- | --
C301 (10 cavities) | Body wiring harness to the left side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C304 (10 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C305 (12 cavities) | Body wiring harness to the electronic brake control wiring harness and fuel sender wiring harness, mounted as a pass through, beneath the vehicle behind the driver seat | Harness Routing Views | Inline Harness Connector End Views
C306 (2 cavities) | Electronic brake control wiring harness to the right rear wheel speed sensor wiring harness, under the right side of the vehicle, front of the right rear wheel | Harness Routing Views | Inline Harness Connector End Views
C308 (23 cavities) | Body wiring harness to the roof wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views | Inline Harness Connector End Views
C309 (2 cavities) | Electronic Brake control wiring harness to the left rear wheel speed sensor wiring harness, under the left side of the vehicle, front of the left rear wheel | Harness Routing Views | Inline Harness Connector End Views
C313 (2 cavities) | Body wiring harness to the driver seat adjuster switch wiring harness, under the driver seat | Harness Routing Views | Inline Harness Connector End Views
C314 (2 cavities) | Body wiring harness to the passenger seat adjuster switch wiring harness, under the passenger seat | Harness Routing Views | Inline Harness Connector End Views
C315 (4 cavities) | Body wiring harness to the driver seat heater module wiring harness, under the driver seat | Harness Routing Views | Inline Harness Connector End Views
C316 (4 cavities) | Body wiring harness to the passenger seat heater module wiring harness, under the passenger seat | Harness Routing Views | Inline Harness Connector End Views
C326 (4 cavities) | Inside overhead console, in front of the video display bracket assembly, tucked underneath the headliner | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
C328 (8 cavities) | Inside overhead console, in front of the video display bracket assembly, tucked underneath the headliner | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
C396 (1 cavity) | Antenna coaxial cable wiring harness to the window radio antenna lead, above the roof headliner, center of the windshield | -- | --
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
C401 (4 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views | Inline Harness Connector End Views
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
C403 (3 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views | Inline Harness Connector End Views
C405 (10 cavities) | Body wiring harness to the auto level control wiring harness, behind the left quarter panel, behind the left rear wheelhouse | Harness Routing Views | Inline Harness Connector End Views
C407 Domestic (6 cavities) | Auto level control wiring harness to the trailer rear wiring harness, beneath the vehicle, near P403, near the left rear wheelhouse | Harness Routing Views | Inline Harness Connector End Views
C407 Export (8 cavities) | Auto level control wiring harness to the trailer rear wiring harness, beneath the vehicle, near P403, near the left rear wheelhouse | Harness Routing Views | Inline Harness Connector End Views
G100 | Battery grounded to the right inner fender, near the battery | Harness Routing Views | --
G101 | Front of the vehicle, right of the left headlamp, on the front upper crossmember | -- | --
G102 | Right side of the engine compartment, right inner fender, near the battery | Harness Routing Views | --
G111 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views | --
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views | --
G114 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views | --
G117 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
G201 | Left side of the IP, secured on the underside of the cross car beam, above the park brake assembly | Harness Routing Views | --
G210 | Left side of the front floor console bracket | Harness Routing Views | --
G301 | Secured to the inside of the lower left B-pillar | Harness Routing Views | --
G302 | Secured near the base of the right B-pillar | Harness Routing Views | --
G390 | Antenna coaxial cable secured with the clamp, grounding the coaxial shield to the top of the windshield frame, right of the mirror | -- | --
G401 | Secured to the lower left D-pillar | -- | --
G402 | Secured to the lower right D-pillar | Harness Routing Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
P400 | Behind the right taillamp | Harness Routing Views | --
P401 | Behind the left taillamp | Harness Routing Views | --
P403 | Behind the left wheelhouse | Harness Routing Views | --
P405 | Between the left side of the liftgate and the roof | Harness Routing Views | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views | --
S105 | Engine harness, top right side radiator approximately 20 cm (8 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S107 | Engine harness, center of the engine approximately 4 cm (2 in) from the camshaft position sensor breakout | -- | --
S108 | Engine harness, front left side of the engine compartment approximately 8 cm (3 in) from the PCM breakout | -- | --
S109 | Fuel injector harness, center of the engine approximately 16 cm (6 in) from C102 | -- | --
S110 | Fuel injector harness, center of the engine approximately 14 cm (4 in) from C102 | -- | --
S115 | Automatic transaxle harness, inside automatic transaxle housing approximately 42 cm (17 in) from the automatic transaxle fluid temperature sensor | -- | --
S122 | Engine harness, top left side of the radiator approximately 25 cm (10 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S123 | Forward lamp harness, right front of the vehicle approximately 10 cm (4 in) from the right fog lamp breakout | -- | --
124 | Forward lamp harness, left front of the vehicle approximately 7 cm (3 in) from the left fog lamp breakout | -- | --
S146 | Engine harness, center of the engine approximately 10 cm (4 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S155 | Engine harness, front of the engine approximately 14 cm (6 in) from the knock sensor breakout | -- | --
S167 | Engine harness, front left side of the engine approximately 5 cm (2 in) PCM breakout | -- | --
S201 | IP harness, right side of the IP approximately 21 cm (8 in) from the radio breakout | -- | --
S202 | IP harness, left side of the IP approximately 15 cm (6 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S203 | IP harness, right side of the IP approximately 9 cm (4 in) from the radio breakout | -- | --
S204 | IP harness, right side of the IP approximately 10 cm (4 in) from the radio breakout | -- | --
S205 | IP harness, left side of the IP approximately 8 cm (3 in) from the hazard lamp/turn signal flasher breakout | -- | --
S207 | IP harness, left side of IP approximately 4 cm (2 in) from the hazard lamp/turn signal flasher breakout | -- | --
S208 | Video entertainment harness | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S210 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S213 | IP harness, center of IP approximately 72 cm (28 in) from the cigar lighter | -- | --
S215 | IP harness, left side of IP approximately 13 cm (5 in) from headlamp switch breakout | -- | --
S219 | IP harness, left side of the IP approximately 10 cm (4 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S221 | IP harness, left side of the IP approximately 4 cm (2 in) from the headlamp switch breakout | -- | --
S223 | IP harness, left side of the IP approximately 6 cm (2 in) from the radio and rear window wiper/washer and multi-function switch breakout | -- | --
S225 | IP harness, center of the IP approximately 8 cm (3 in) | -- | --
S227 | Video entertainment harness behind right side of hush panel | -- | --
S228 | IP harness, right side of the IP approximately 19 cm (7 in) from the radio breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S232 | IP harness, right side of the IP approximately 17 cm (7 in) from the radio breakout | -- | --
S233 | IP harness, left side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S235 | IP harness, left side of the IP approximately 21 cm (8 in) from P101 | -- | --
S236 | Below left side of IP, near park brake | -- | --
S237 | IP harness, right side of the IP approximately 4 cm (2 in) from the C203 breakout | -- | --
S238 | IP harness, center of the IP approximately 80 cm (31 in) from the cigar lighter connector | -- | --
S239 | IP harness, right side of the IP approximately 8 cm (3 in) from the C203 breakout | -- | --
S242 | IP harness, left side of the IP approximately 14 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S243 | IP harness, center of the IP approximately 37 cm (15 in) from the radio and rear window wiper/washer and multi-function switch breakout | -- | --
S245 | IP harness, right side of the IP approximately 5 cm (2 in) from the radio breakout, within the radio breakout | -- | --
S247 | IP harness, center of the IP approximately 31 cm (12 in) from the radio | -- | --
S249 | IP harness, right side of the IP approximately 14 cm (6 in) from P100 | -- | --
S252 | IP harness, center of the IP approximately 76 cm (30 in) from the cigar lighter | -- | --
S259 | IP harness, right side of the IP approximately 3 cm (1 in) from the cigar lighter breakout | -- | --
S261 | IP harness, right side of the IP at the electric air inlet actuator breakout | -- | --
S262 | IP harness, right side of the IP approximately 4 cm (2 in) from the blower motor resistor breakout | -- | --
S263 | IP harness, right side of the IP at the electric air inlet actuator breakout | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S266 | IP harness, left side of the IP approximately 24 cm (9 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S268 | IP harness, right side of the IP approximately 29 cm (11 in) from the relay center breakout | -- | --
S270 | IP harness, right side of the IP approximately 6 (2 in) from the relay center breakout | -- | --
S272 | IP harness, right side of the IP approximately 2 cm (1 in) from the relay center breakout | -- | --
S274 | IP harness, right side of the IP approximately 4 cm (2 in) from the BCM breakout | -- | --
S275 | IP harness, right side of the IP approximately 6 cm (2.5 in) from the BCM breakout | -- | --
S276 | IP harness, right side of the IP approximately 8 cm (3 in) from the BCM breakout | -- | --
S278 | IP harness, right side of the IP approximately 12 cm (5 in) from the BCM breakout | -- | --
S279 | IP harness, right side of the IP approximately 12 cm (5 in) from the hazard lamp/turn signal flasher breakout | -- | --
S280 | IP harness, right side of the IP approximately 10 cm (4 in) from P100 | -- | --
S282 | IP harness, left side of the IP approximately 4 cm (2 in) from the cigar lighter breakout | -- | --
S284 | IP harness, right side of the IP approximately 6 cm (2 in) from P100 | -- | --
S301 | Roof harness, approximately 65 cm (24 in) from the driver information display breakout | -- | --
S302 | Body harness, right front door approximately 7 cm (3 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S304 | Body harness, right front door approximately 28 cm (11 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S305 | Dome lamp wiring harness to body wiring harness, approximately 30 cm (12 in) from driver information display | -- | --
S307 | Boyd harness, right front door approximately 4 cm (2 in) from C302 breakout | -- | --
S308 | Body harness, left front door approximately 39 cm (15 in) from the seat belt switch breakout | -- | --
S309 | Body harness, forward of the right front door approximately 7 cm (3 in) from the C302 breakout | -- | --
S311 | Body harness, under the right front door sill approximately 13 cm (5 in) from the C302 breakout | -- | --
S312 | Body harness, front of the right hand B-pillar approximately 31 cm (12 in) front of the inflatable restraint sensing and diagnostic module breakout | -- | --
S314 | Body harness, under the right front seat approximately 2 cm (1 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S315 | Body harness, under the right front seat approximately 8 cm (3 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S316 | Body harness, front of the right B-pillar approximately 34 cm (13 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S317 | Body harness, under right front door sill, approximately 17 cm (7 in) from C302 breakout | -- | --
S318 | Body harness, under the right front door sill approximately 17 cm (7 in) C302 breakout | -- | --
S319 | Body harness, under the right front door sill approximately 17 cm (7 in) C302 breakout | -- | --
S320 | Body harness, near the base of the right B-pillar approximately 33 cm (13 in) forward of the right door lock switch plate (pillar mounted, plunger) breakout | -- | --
S323 | Body harness, under the left front seat approximately 7 cm (3 in) from the seat belt switch breakout | -- | --
S324 | Body harness, top/forward area of the left rear wheel well approximately 5 cm (2 in) behind the second oval clamp | -- | --
S325 | Body harness, front of the left B-pillar approximately 7 cm (3 in) from the left sliding door jamb switch breakout | -- | --
S326 | Body harness, top/forward area of the left rear wheel well approximately 13 cm (5 in) behind the second oval clamp | -- | --
S327 | Body harness, under the left front seat approximately 13 cm (5 in) from the seat belt switch breakout | -- | --
S328 | Body harness, between the left D-pillar and the wheel well approximately 32 cm (13 in) forward of the G401 breakout | -- | --
S329 | Fuel sender harness, between C305 and the fuel tank approximately 20 cm (8 in) from C305 | -- | --
S330 | Body harness, left of B-pillar, approximately 40 cm (16 in) from seat belt switch breakout | -- | --
S331 | Body harness, front of the left B-pillar approximately 59 cm (23 in) from the G301 breakout | -- | --
S333 | Body harness, front of the left B-pillar approximately 39 cm (15 in) from the G301 breakout | -- | --
S337 | Body harness, rear of the left B-pillar base approximately 8 cm (3 in) from the P401 breakout | -- | --
S339 | Body harness, front of the left B-pillar approximately 26 cm (10 in) from the G301 breakout | -- | --
S341 | Body harness, in front of the left wheelhouse approximately 13 cm (5 in) from the radio rear speaker amplifier breakout | -- | --
S343 | Body harness, in front of the left wheelhouse approximately 40 cm (16 in) from the radio rear speaker amplifier breakout | -- | --
S345 | Body harness, in front of the left rear wheelhouse approximately 48 cm (19 in) from the left sliding door jamb switch | -- | --
S350 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 12.7 cm (5 in) from the connector for the Seat Heater Module--Driver. | -- | --
S351 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 2.5 cm (1 in) from the connector for the Seat Heater Module--Driver. | -- | --
S352 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 12.7 cm (5 in) from the connector for the Seat Heater Module--Driver. | -- | --
S353 | In the Pigtail for the Heater--Seat Cusion--Driver, approximately 2.5 cm (1 in) from the connector for the Seat Heater Module--Driver. | -- | --
S390 | Roof harness, overhead console approximately 10 cm (4 in) from the right sunshade lighted vanity mirror breakout | -- | --
S392 | Roof harness, right B-pillar approximately 27 cm (10 in) from the power sliding door open/close switch (right B-pillar) | -- | --
S393 | Roof harness, right side of the overhead console approximately 20 cm (8 in) from the G302 breakout | -- | --
S395 | Roof harness, right side of the overhead console approximately 13 cm (5 in) from the he power sliding door open/close switch (right B-pillar) breakout | -- | --
S397 | Roof harness, right side of the overhead console approximately 7 cm (3 in) from the G302 breakout | -- | --
S399 | Sunroof harness, front of the overhead console approximately 10 cm (4 in) from the sunroof control module | -- | --
S403 | Body harness, left rear of the body on top of the wheel well approximately 13 cm (5 in) from the top and rear clips | -- | --
S405 | Body harness, left rear of the body approximately 4 cm (2 in) from the P401 breakout | -- | --
S406 | Body harness, left rear of the body approximately 17 cm (7 in) from the P401 breakout | -- | --
S407 | Body harness, left rear of the body approximately 13 cm (5 in) from the P401 breakout | -- | --
S409 | Body harness, left rear of the body approximately 7 cm (3 in) from the P401 breakout | -- | --
S411 | Body harness, left rear of the body approximately 7 cm (3 in) from the P401 breakout | -- | --
S412 | Body harness, left rear of the body approximately 8 cm (3.5 in) from the P401 breakout | -- | --
S415 | Body harness, left rear of the body approximately 11 cm (4 in) from the P401 breakout | -- | --
S419 | Body harness, left rear of the body approximately 21 cm (8 in) from the P401 breakout | -- | --
S423 | Body harness, left rear of the body approximately 54 cm (20 in) from the C403 breakout | -- | --
S427 | Body harness, left rear of the body approximately 41 cm (16 in) from the C403 breakout | -- | --
S431 | Body harness, left rear of the body approximately 4 cm (2 in) from the P401 breakout | -- | --
S435 | Body harness, left rear of the body approximately 26 cm (10 in) from the P401 breakout | -- | --
S440 | Auto level control harness, left rear of the body approximately 24 cm (9 in) from P403 | -- | --
S441 | Auto level control harness, left rear of the body approximately 24 cm (9 in) from P403 | -- | --
S443 | Auto level control harness, left rear of the body approximately 20 cm (8 in) from P403 | -- | --
S445 | Auto level control harness, left rear of the body approximately 16 cm (6 in) from P403 | -- | --
S457 | Liftgate harness, center of the liftgate approximately 7 cm (3 in) from the liftgate lock (door ajar switch) breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the liftgate lock cylinder switch breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --
S506 | Left door harness, left door approximately 35 cm (3 in) from the left window switch | -- | --
S604 (w/AB5) | Right door harness, right door approximately 10 cm (4 in) from the right window switch breakout | -- | --
S604 (w/o AB5) | Right door harness, between P600 and the right front speaker breaker | -- | --
S606 | Right door harness, right door approximately 35 cm (13 in) from the right window switch | -- | --
S817 | Sliding door harness, inside the right rear side door approximately 11 cm (4 in) from the right rear door latch release actuator breakout | -- | --