For 1990-2009 cars

### Removal Procedure

1. Remove the left side instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
2. Disconnect the electrical connectors from the stop light switch.
3. Remove the stop lamp switch (1) from the brake pedal bracket (2).

### Installation Procedure

1. Install the stop lamp switch (1) to the brake pedal bracket (2).
2. Connect the electrical connectors to the stop light switch.
3. Install the left side instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
4. Adjust the stop lamp switch. Refer to Stop Lamp Switch Adjustment .