For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door conduit. Refer to Front Side Door Conduit Replacement .
4. Remove the front door window belt inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
5. Remove the front door window weatherstrip. Refer to Front Side Door Window Weatherstrip Replacement .
6. Remove the front door window. Refer to Front Side Door Window Replacement .
7. Remove the outside rearview mirror. Refer to Power Mirror Replacement .
8. Remove the front door module. Refer to Front Door Module Replacement .
9. Remove the front door outside handle. Refer to Front Side Door Outside Handle Replacement .
10. Remove the front door lock. Refer to Front Side Door Lock Replacement .
11. Remove the front door window belt outer sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
12. Remove the front door window run channel. Refer to Front Side Door Window Channel Replacement .
13. Remove the front door molding. Refer to Door Body Side Molding Replacement in Exterior Trim.
14. Remove the front door hinges. Refer to Front Side Door Hinge Replacement .
15. Remove the front door from the body.

### Installation Procedure

1. Install the front door to the body.
2. Install the front door hinges. Refer to Front Side Door Hinge Replacement .
3. Install the front door molding. Refer to Door Body Side Molding Replacement in Exterior Trim.
4. Install the front door window run channel. Refer to Front Side Door Window Channel Replacement .
5. Install the front door window belt outer sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
6. Install the front door lock. Refer to Front Side Door Lock Replacement .
7. Install the front door outside handle. Refer to Front Side Door Outside Handle Replacement .
8. Install the front door module. Refer to Front Door Module Replacement .
9. Install the outside rearview mirror. Refer to Power Mirror Replacement .
10. Install the front door window. Refer to Front Side Door Window Replacement .
11. Install the front door window weatherstrip. Refer to Front Side Door Window Weatherstrip Replacement .
12. Install the front door window belt inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
13. Install the front door conduit. Refer to Front Side Door Conduit Replacement .
14. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
15. Refer to front door trim panel. Refer to Door Trim Panel Replacement .
16. Adjust the front door. Refer to Front Side Door Adjustment .