For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views | Body Control System Connector End Views
Horn Switch | Behind the inflatable restraint steering wheel module | SIR Component Views | --
Inflatable Restraint Steering Wheel Module | Center of the steering wheel, includes the horn switches | SIR Component Views | SIR Connector End Views
Inflatable Restraint Steering Wheel Module Coil | Center of the steering wheel, behind the inflatable restraint steering wheel module | SIR Component Views | SIR Connector End Views
Left Horn | Front left side of the vehicle, mounted to the left side of the front lower crossmember | Horn Component Views | Horn Connector End Views
Right Horn | Front right side of the vehicle, mounted to the right side of the front lower crossmember | Horn Component Views | Horn Connector End Views
Turn Signal and Headlamp Dimmer Switch and Windshield Wiper and Windshield Washer Switch | Inside the steering column | Lighting Systems Component Views | Lighting Systems Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views | Inline Harness Connector End Views
G101 | Front of the vehicle, right of the left headlamp, on the front upper crossmember | -- | --
G102 | Right side of the engine compartment, right inner fender, near the battery | Harness Routing Views | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
S123 | Forward lamp harness, right front of the vehicle approximately 10 cm (4 in) from the right fog lamp breakout | -- | --
124 | Forward lamp harness, left front of the vehicle approximately 7 cm (3 in) from the left fog lamp breakout | -- | --
S213 | IP harness, center of IP approximately 72 cm (28 in) from the cigar lighter | -- | --