For 1990-2009 cars

DTC | Description
--- | ---
U1000 | Class 2 Communication Malfunction. Refer to DTC U1000 and DTC U1255 Class 2 Communication Malfunction .
U1016 | Lost Communication with PCM. Refer to DTC U1001-U1254 Lost Communication with XXX .
U1040 | Lost Communication with ABS. Refer to DTC U1001-U1254 Lost Communication with XXX .
U1088 | Lost Communication with SIR. Refer to DTC U1001-U1254 Lost Communication with XXX .
U1096 | Lost Communication with IPC. Refer to DTC U1001-U1254 Lost Communication with XXX .
U1192 | Lost Communication with PK3. Refer to DTC U1001-U1254 Lost Communication with XXX .
U1255 | Class 2 Communication Malfunction. Refer to DTC U1000 and DTC U1255 Class 2 Communication Malfunction .
U1300 | Class 2 Data Link Low. Refer to DTC U1300 Class 2 Data Link Low .
U1301 | Class 2 Data Link High. Refer to DTC U1301 Class 2 Data Link High .
U1305 | Class 2 Data Link Low or High. Refer to DTC U1305 Class 2 Data Link Low or High .