For 1990-2009 cars

### Removal Procedure

1. Position the windshield wiper arms to the up position.
2. Remove the retainers (1) from the air inlet grille to the body.
3. Partially remove the air inlet grille from the body.
4. Remove the washer hose from the air inlet grille.

### Installation Procedure

1. Install the air inlet grille to the body.
2. Install the air inlet grille retainers (1).
3. Position the windshield wiper arms to the down position.