For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Center Air Distribution Extension Duct Nuts | 10 N·m | 89 lb in
Cross Car Beam Bolts/Screws | 25 N·m | 18 lb ft
Data Link Connector Bolts/Screws | 2 N·m | 18 lb in
Defroster Duct Bolts/Screws | 10 N·m | 89 lb in
Driver Information Display to Overhead Console Bolts | 1 N·m | 9 lb in
Front Floor Console Bracket Bolts/Screws | 2.5 N·m | 22 lb in
Front Floor Console Bracket Lower Nuts | 10 N·m | 89 lb in
Front Floor Console Upper Bolts/Screws | 2.5 N·m | 22 lb in
Heater A/C Controls Bolts/Screws | 2.5 N·m | 22 lb in
Hood Release Handle Bolts/Screws | 2 N·m | 18 lb in
Instrument Panel Accessory Trim Plate Screws | 2 N·m | 18 lb in
Instrument Panel Bolts/Screws | 10 N·m | 89 lb in
Instrument Panel Cluster Screws | 2.5 N·m | 22 lb in
Instrumetn Panel Compartment Latch Screws | 1 N·m | 9 lb in
Instrument Panel Compartment Screws | 2.5 N·m | 22 lb in
Instrument Panel Lower Brace Bolts/Screws | 2 N·m | 18 lb in
Knee Bolster Bolts/Screws | 2.5 N·m | 22 lb in
Outside Ambient Air Temperature Sensor to Radiator Support Bolt | 2 N·m | 18 lb in
Radio Bolts/Screws | 2.5 N·m | 22 lb in
Switch Bank Bolts/Screws | 2.5 N·m | 22 lb in