For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the auxiliary water deflector.

### Installation Procedure

1. Install the auxiliary water deflector.
2. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Install the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .