For 1990-2009 cars

### Removal Procedure

Important: This vehicle contains 2 antenna cables. These procedures are applicable to both of the antenna cables.

1. Remove the radio. Refer to Radio Replacement .
2. Remove the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.
3. Remove the right cowl side trim panel. Refer to Cowl Side Trim Panel Replacement in Interior Trim.
4. Remove the headliner front. Refer to Headlining Trim Panel Replacement in Interior Trim.
5. Remove the antenna cable extension to roof bolt.
6. Remove the antenna cable from the instrument panel carrier.
7. Remove the following components from the vehicle:

• | The antenna cable

• | The antenna cable extension

### Installation Procedure

1. Install the following components to the vehicle:

• | The antenna cable

• | The antenna cable extension

2. Install the antenna cable to the instrument panel carrier.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the antenna cable extension to roof bolt.

Tighten
Tighten the bolt to 3.2 N·m (28 lb in).

4. Install the headliner front. Refer to Headlining Trim Panel Replacement in Interior Trim.
5. Install the right cowl side trim panel. Refer to Cowl Side Trim Panel Replacement in Interior Trim.
6. Install the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.
7. Install the radio. Refer to Radio Replacement .