For 1990-2009 cars

## Door Sill Plate Replacement Door

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

Use J 38778 in order to remove the door-opening carpet retainers from the carpet retainer.

### Installation Procedure

Push the door-opening carpet retainers to the retainer support.

## Door Sill Plate Replacement Sliding Door

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

Remove the sliding door-opening carpet retainer (1) from the carpet retainer(s) support using the J 38778 .

### Installation Procedure

Push the sliding door-opening carpet retainer(s) (1) to the retainer support.