For 1990-2009 cars

#### Engine Coolant Fan Motor 1 (RH)

Connector Part Information |

• | 12085030

• | 2-Way F Metri-Pack 630 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 504 | Ground
B | GRY | 532 | Engine coolant fan 1 (RH) feed

#### Engine Coolant Fan Motor 2 (RH)

Connector Part Information |

• | 12085030

• | 2-Way F Metri-Pack 630 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1050 | Ground
B | LT BLU | 409 | Engine coolant fan 2 (LH) feed

#### Engine Coolant Level Module

Connector Part Information |

• | 12162185

• | 3-Way F Metri-Pack 150.1 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | YEL/BLK | 68 | Low coolant level control circuit
C | BLK/WHT | 451 | Engine coolant level module Ground