For 1990-2009 cars

### Removal Procedure

1. Remove the front door lock module. Refer to Front Door Module Replacement .
2. Remove the front door lock from the front door lock module bracket.
3. Disconnect the front door inside handle rods from the front door lock.

### Installation Procedure

1. Position the front door lock to the front door lock module.
2. Install the front door lock to the door lock module bracket.
3. Connect the front door inside handle rods.
4. Install the front door lock module. Refer to Front Door Module Replacement .