For 1990-2009 cars

## Fog Lamp Indicator Always On Domestic

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the lighting diagnostic system check? | -- | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 | Do the front fog lamps operate properly? | -- | Go to Step 3 | Go to Fog Lamps Always On
3 | Replace the IPC. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges, and Console. Important: Perform the set up procedure for the IP. Did you complete the replacement and the set up procedure? | -- | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2