For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Auxiliary Video Module (AVM) | Overhead console, left side of video screen | Entertainment Component Views | Entertainment Connector End Views
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Front Door Speakers | Inside the front door | -- | Entertainment Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Headlamp and IP Lamp Dimmer Switch | Left of the instrument cluster | Lighting Systems Component Views | --
Inflatable Restraint Steering Wheel Module Coil | Center of the steering wheel, behind the inflatable restraint steering wheel module | SIR Component Views | SIR Connector End Views
Interface Module (IM) | Inside overhead console, left corner | Entertainment Component Views | Entertainment Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Radio | Center of the IP console | Entertainment Component Views | Entertainment Connector End Views
Radio Control Switches | Left and right sides of the inflatable restraint steering wheel module | Entertainment Component Views | --
Radio Liftgate Speakers | On both sides of the liftgate | Entertainment Component Views | Entertainment Connector End Views
Radio Rear Seat Audio Control (4 Door) | Part of the left rear armrest | HVAC Component Views | Entertainment Connector End Views
Radio Rear Seat Audio Control (5 Door) | Part of the rear roof console, above the driver seat | HVAC Component Views | Entertainment Connector End Views
Radio Rear Seat Audio Control (WU3) | Part of the rear roof console, above the right passenger seat | HVAC Component Views | Entertainment Connector End Views
Second Seat Audio (SSA) Control | Overhead console, right side of video screen | HVAC Component Views | Entertainment Connector End Views
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Tape Retract Module (TRM) | Underneath left side instrument panel, near left side of the Data Link Connector (DLC), taped to the VCP harness | Entertainment Component Views | Entertainment Connector End Views
Third Seat Audio (TSA) Control | Right quarter trim panel, next to the third row right seat | Entertainment Component Views | Entertainment Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
Video Cassette Player (VCP) | Front floor console | Entertainment Component Views | --
Video Screen-Liquid Crystal Display (LCD) | In the center of the overhead console | HVAC Component Views | --
Windshield Antenna | Within the windshield | -- | --
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C205 (4 cavities) | IP wiring harness to the steering wheel radio control wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views | Inline Harness Connector End Views
C290 (1 cavity) | Antenna coaxial cable wiring harness to the antenna coaxial cable wiring harness, behind the IP compartment | -- | --
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views | Inline Harness Connector End Views
C308 (23 cavities) | Body wiring harness to the roof wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views | Inline Harness Connector End Views
C326 (4 cavities) | Inside overhead console, in front of the video display bracket assembly, tucked underneath the headliner | Entertainment Component Views | Entertainment Connector End Views
C328 (8 cavities) | Inside overhead console, in front of the video display bracket assembly, tucked underneath the headliner | Entertainment Component Views | Entertainment Connector End Views
C396 (1 cavity) | Antenna coaxial cable wiring harness to the window radio antenna lead, above the roof headliner, center of the windshield | -- | --
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
G201 | Left side of the IP, secured on the underside of the cross car beam, above the park brake assembly | Harness Routing Views | --
G210 | Left side of the front floor console bracket | Harness Routing Views | --
G390 | Antenna coaxial cable secured with the clamp, grounding the coaxial shield to the top of the windshield frame, right of the mirror | -- | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views | --
S202 | IP harness, leftt side of the IP approximately 15 cm (6 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S203 | IP harness, right side of the IP approximately 9 cm (4 in) from the radio breakout | -- | --
S223 | IP harness, left side of the IP approximately 6 cm (2 in) from the radio and rear window wiper/washer and multi-function switch breakout | -- | --
S225 | IP harness, center of the IP approximately 8 cm (3 in) | -- | --
S227 | Video entertainment harness behind right side of hush panel | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S242 | IP harness, left side of the IP approximately 14 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S247 | IP harness, center of the IP approximately 31 cm (12 in) from the radio | -- | --
S316 | Body harness, front of the right B-pillar approximately 34 cm (13 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S320 | Body harness, near the base of the right B-pillar approximately 33 cm (13 in) forward of the right door lock switch plate (pillar mounted, plunger) breakout | -- | --
S331 | Body harness, front of the left B-pillar approximately 59 cm (23 in) from the G301 breakout | -- | --