For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer Rear System Check? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check
2 |

1. Disconnect the rear wiper/washer switch connector C1.
2. Turn the ignition switch to RUN.

Does the wiper operate?

--

Go to Step 4

Go to Step 3

3 | Replace the rear wiper/washer switch. Refer to Multifunction Switch Assembly Replacement - Instrument Panel in Lighting Systems. Did you complete the replacement? | -- | Go to Step 6 | --
4 | Inspect for a short to voltage in CKT 391 or CKT 392. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 6 | Go to Step 5
5 | Replace the rear wiper motor. Refer to Rear Window Wiper Motor Replacement . Did you complete the replacement? | -- | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Wiper/Washer Rear System Check