For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the rear storage compartment by turning the knob counterclockwise to release.
3. Lift up and pull to release the storage compartment from the vehicle.

### Installation Procedure

1. Install the storage compartment by sliding the compartment toward the rear seats until fully inserted.
2. Turn the knob clockwise until tight.
3. Close the liftgate.