For 1990-2009 cars

Table 1: | Driver Information Display
Table 2: | Instrument Cluster Connector C1
Table 3: | Instrument Cluster Connector C2

#### Driver Information Display

Connector Part Information |

• | 1206-4980

• | 9-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | BRN | 241 | Fused Input Feed
8 | BLK | 1550 | Ground
9 | -- | -- | Not Used
10 | LT GRN/BLK | 735 | Outside Ambient Air Temperature Sensor Signal Input
11 | GRY | 8 | Interior Lamps Dimming Input Feed
12 | GRY/BLK | 308 | Audio Switch Signal Input
13 | -- | -- | Not Used
14 | ORN | 640 | Fused Input Feed
15 | YEL | 1127 | Class 2 Serial Data Line

#### Instrument Cluster Connector C1

Connector Part Information |

• | 1206-4799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1450 | Ground
B | YEL | 18 | Left Turn Indicator Input
C | DK GRN | 19 | Right Turn Indicator Input
D | LT GRN | 11 | High Beam Indicator Input
E | DK GRN/WHT | 529 | Seat Belt Indicator
F | YEL | 804 | Door Ajar Input
G | BRN | 996 | Trailer Towing Indicator Input
H | PPL | 34 | Fog Lamp Input
J | YEL/BLK | 68 | Low Coolant Level Indicator Input
K | DK BLU/WHT | 9804 | Hatch Ajar Input
L | RED/WHT | 9901 | BCM Chime Request
M | GRY | 8 | Interior Lamps Dimming Input Feed

#### Instrument Cluster Connector C2

Connector Part Information |

• | 1206-4799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1550 | Ground
B | -- | -- | Not Used
C | PNK | 1020 | Fused Input Feed
D | YEL | 43 | Fused Input Feed
E | PPL | 209 | Brake Fluid Level Indicator Input
F | GRY | 1036 | Class 2 Serial Data Line
G | BRN/WHT | 419 | Service Engine Soon Indicator
H | DK GRN/WHT | 9902 | BCM CTD Disarm (+UA6)
J | PNK | 39 | Fused Input Feed
K | BLK | 707 | RAP Relay Feed
L | TAN/WHT | 33 | Park Brake Input
M | ORN | 2940 | Fused Input Feed