For 1990-2009 cars

Table 1: | Underhood Accessory Wiring Junction Block Maxifuse® Application Table
Table 2: | Fuse Block Application Table

### Underhood Accessory Wiring Junction Block

### Underhood Accessory Wiring Junction Block Label

#### Underhood Accessory Wiring Junction Block Maxifuse® Application Table

Fuse | Rating | Description
--- | --- | ---
1-COOL FAN 2 | 30A | Coolant Fans
3-HEADLAMPS | 60A | Circuit Breakers:

• | FRT HVAC HI BLWR Fuse (IP)

• | HEADLAMP Fuse (IP):

- | HAZARD

- | PASS KEY

- | STOP LAMP

4-BATT MAIN 2 | 60A | Circuit Breaker:

• | PWR HEATED SEAT/PSD Fuses (IP)

• | ELC/TRAILER

• | RR DEFOG/HTD MIRRORS

• | RR FOG LP

• | RR DEFOG LP

5-IGN MAIN 1 | 40A | Ignition Switch to Fuses (IP):

• | PCM/ABS

• | CAN VENT SOL

• | DRL

• | PCM/CRANK

• | IGN 1

• | SIR

• | T/SIG

• | CRUISE

• | PCM/PASS KEY/CLUSTER

6-COOL FAN 1 | 30A | Coolant Fans
7-BATT MAIN 1 | 60A | Fuses (IP):

• | CLUSTER BATT

• | CIGAR/DLC

• | CTSY LAMP

• | RAP RELAY

• | FRT PWR SCKT

• | PWR LOCK

• | PWR MIRROR

• | RIGHT REAR PWR SCKT

8-IGN MAIN 2 | 60A | Ignition Switch to Fuses (IP):

• | BCM PRGRM

• | RR WPR/WSHR

• | FRT/WPR/WSHR

• | MALL/CLUSTER

• | RAP RELAY

• | PWR OTR VENT

• | HVAC/DIC/DRL/HEATED SEAT

• | HVAC BLOWER

• | RR HVAC

• | TEMP CONT

• | PWR WDO Circuit Breaker

18-INJ | 10A | Fuel Injectors 1-6
21-IGNI-UH | 15A |

• | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

• | Heated Oxygen Sensor #1, AND #2

• | Mass Air Flow (MAF) Sensor

• | Air Injection BL Valve

25-ELEK IGN | 15A | Ignition Control Module (ICM)
27-B/U LAMP | 10A | Transaxle Range Switch to Backup Lamps
28-A/C CLU | 10A | A/C CLU Relay to A/C Compressor Clutch Coil
29-RADIO | 10A |

• | Driver Information Display

• | Heater-A/C Control

• | Radio Rear Side Door Actuator Control Module

• | Remote Control Door Lock Receiver (RCDLR)

• | Security Indicator Lamp

• | Theft Deterrent Shock Sensor

30-ALT SENSE | 10A | Generator
31-TCC | 10A |

• | Automatic Transaxle (Torque Converter Clutch and Shift Solenoids)

• | Stop Lamp Switch to Powertrain Control Module (PCM)

32-FUEL PUMP | 15A | Fuel Pump Relay
33-ECM SENSE | 10A | Powertrain Control Module (PCM)
35-FOG LP | 10A | Fog Lamp Relay
36-HORN | 15A | Horn Relay
37-PARK LP | 20A |

• | Daytime Running Lamps (DRL) Control Module

• | Headlamp and IP Lamp Dimmer Switch

• | Theft Deterrent Relay to Headlamps

39-AIR | 30A | Air Pump Relay

### Instrument Panel Fuse Block

#### Fuse Block Application Table

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---
BCM PRGRM | 10A | Body Control Module (BCM)
CAN VENT SOL | 10A | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
CIGAR/DLC | 15A |

• | Cigar Lighter

• | Data Link Connector (DLC)

CLUSTER/BATT | 10A | Instrument Cluster
CRUISE | 10A |

• | Cruise Control Module

• | Cruise Control Release Switch

• | Cruise Control Switch

CTSY LAMP | 10A | Body Control Module (BCM)
DRL | 10A | Daytime Running Lamps (DRL) Control Module
ELC/TRAILER | 25A | Auto Level Control (ALC) air Compressor, Automatic Level on (ALC) In
FRT PWR SCKT | 20A | Front Electric Accessory Plug Housing
FRT WPR/WSHR | 25A |

• | Windshield Wiper Motor

• | Windshield Wiper/Washer Switch

HAZARD | 15A |

• | Turn Signal Switch

• | Trailer Towing Indicator

HTD MIRROR | 10A | LH, RH Outside Rearview Mirrors
HVAC/BLOWER | 25A | Heater-A/C Control
HVAC/DIC/DRL/HEATED SEAT | 10A |

• | Electric Slave Actuator

• | Heater A/C Control

• | Electric Air Inlet Actuator

• | Rear Window Defogger Relay

• | Heated Seat Switch

• | Driver Information Display (DID)

• | Daytime Running Lamps (DRL) Control Module

IGNI | 10A |

• | Body Control Module (BCM)

• | Instrument Cluster

• | Rear Side Door Actuator Control Module

• | Stop Lamp Switch

LH HEADLP HIGH | 10A | LH Headlamp High Beam
LH HEADLP LOW | 10A |
LH T/LP | 10A |

• | LH Taillamp

• | Trailer Rear Wiring Harness

MALL/CLUSTER | 10A |

• | Body Control Module (BCM)

• | Instrument Cluster

PASS KEY | 10A | Pass Key III Module
PCM/ABS | 10A |

• | Underhood Accessory Wiring Junction Block

• | Transaxle Range Switch

• | Powertrain Control Module (PCM)

• | Electronic Brake Control Module (EBCM)

PCM/CRANK | 10A | Powertrain Control Module (PCM)
PCM/PASS KEY/CLUSTER | 10A |

• | Pass Key III Module

• | Instrument Cluster

• | Powertrain Control Module

PWR LOCK | 20A | Body Control Module (BCM)
PWR MIRROR | 10A | Outside Rearview Mirror Remote Control Switch
PWR QTR VENT | 10A |

• | Interior Lamps

• | Multifunction Switch (Rear Quarter Window Switch)

• | Auto Level Control (ALC) Sensor

• | Auto Level Control (ALC) Air Compressor

RAP RELAY | 10A | Rap Relay
RH HEADLP HIGH | 10A | RH Headlamp High Beam
RH HEADLP LOW | 10A | RH Headlamp Low Beam
RR HVAC/TEMP CONT | 25A |

• | Auxiliary Blower Motor

• | Auxiliary Heater-A/C Control

• | Auxiliary Temperature Valve Actuator

RR DEFOG/HTD MIRRORS | 30A | Rear Window Defogger Relay
RR FOG LP | 10A | Rear Fog Lamp Relay
RR PWR SCKT | 20A | Rear Electric Accessory Plug Housing
RH T/LP | 10A |

• | RH Taillamp

• | Trailer Rear Wiring Harness

RR WPR/WSHR | 20A |

• | Rear Window Wiper Motor

• | Rear Window Wiper/Washer

• | Multifunction Switch (Rear Window Wiper/Washer Switch)

SIR | 15A | Inflatable Restraint Sensing and Diagnostic Module (SDM)
STOP LAMP | 15A | Stop Lamp Switch to Stop Lamps
SWC BACKLIGHT | 2A |

• | Left Hand Radio Control Switch

• | Right Hand Radio Control Switch (Illumination)

T/SIG | 10A | Turn Signal Switch and Backup Lamp Relay