For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Interior Lamp and Multi-function Switch | Center in front of the roof headliner | Lighting Systems Component Views | Lighting Systems Connector End Views
Interior Lamp and Multi-function Switch (Rear Quarter Window Switch) | Part of the interior lamp and multi-function switch | Lighting Systems Component Views | Power Door Systems Connector End Views
Liftgate Door Lock | Inside the liftgate, below the license plate | Body Rear End Component Views | Body Rear End Connector End Views
Liftgate Door Lock (Ajar Indicator Switch) | Part of the liftgate door lock | Body Rear End Component Views | Body Rear End Connector End Views
Rear Quarter Window Actuator | Rear part of the rear quarter window, on the D-pillar | Power Door Systems Component Views | Power Door Systems Connector End Views
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C308 (23 cavities) | Body wiring harness to the roof wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views | Inline Harness Connector End Views
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | -- | Inline Harness Connector End Views
C403 (3 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views | Inline Harness Connector End Views
G302 | Secured near the base of the right B-pillar | Harness Routing Views | --
G401 | Secured to the lower left D-pillar | -- | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views | --
S317 | Body harness, under right front door sill, approsimately 17 cm (7 in) from C302 breakout | -- | --
S390 | Roof harness, overhead console approximately 10 cm (4 in) from the right sunshade lighted vanity mirror breakout | -- | --
S423 | Body harness, left rear of the body approximately 54 cm (20 in) from the C403 breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the liftgate lock cylinder switch breakout | -- | --