For 1990-2009 cars

#### Ashtray Lamp Connector

Connector Part Information |

• | 12124722

• | W2 Axial Type Lamp Socket Wedge Base (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 150 | Ground

#### Backup Lamp Relay

Connector Part Information |

• | 12110541

• | 6-Way F Metri-Pack 280 Series Flexlock (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PNK | 539 | Fused ignition 1 feed
A2 | LT GRN/BLK | 24 | Backup lamp signal
B1-B2 | -- | -- | Not Used
C1 | LT GRN/BLK | 924 | Backup lamp feed
C2 | BLK | 1450 | Ground

#### Cargo Lamp

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### Center High Mounted Stop Lamp (CHMSL)

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 17 | Stop lamp switch output
B | BLK | 450 | Ground

#### Daytime Running Lamps (DRL) Ambient Light Sensor

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 1137 | Daytime running lamp ambient light sensor signal
B | YEL/BLK | 1138 | Daytime running lamp ambient light sensor return

#### Daytime Running Lamps (DRL) Control Module C1

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1340 | Fused battery feed
B | LT BLU | 14 | Turn signal lamp feed-left front
C | DK BLU | 15 | Turn signal lamp feed-right front
D | ORN | 2340 | Fused battery feed
E | LT BLU/WHT | 1414 | Turn signal lamp feed-left front
F | YEL | 10 | Headlamp switch output
G | DK BLU/WHT | 1415 | Turn signal lamp feed-right front
H | BRN | 9 | Park lamp feed

#### Daytime Running Lamps (DRL) Control Module C2

Connector Part Information |

• | 12064766

• | 8-Way F Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1450 | Ground
B | -- | -- | Not Used
C | PNK | 1839 | Fused ignition 1 feed
D | TAN/WHT | 33 | Brake warning indicator lamp output
E | LT BLU | 1134 | Park brake switch signal
F | BRN | 241 | Fused ignition 3 feed
G | YEL/BLK | 1138 | Daytime running lamp ambient light sensor return
H | LT GRN/BLK | 1137 | Daytime running lamp ambient light sensor signal

#### Dome Lamp

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### Hazard Lamp/Turn Signal Flasher

Connector Part Information |

• | 12110541

• | 6-Way F Metri-Pack 280 Series Flexlock (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 1508 | Hazard lamp/turn signal flasher red
A2 | -- | -- | Not Used
B1 | -- | -- | Not Used
B2 | BLK | 1450 | Ground
C1 | PPL | 16 | Turn signal flasher output
C2 | -- | -- | Not Used

#### Headlamp and I/P Lamp Dimmer Switch

Connector Part Information |

• | 12059993

• | 17-Way Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1450 | Ground
B | WHT | 156 | Courtesy lamp output
C-F | -- | -- | Not Used
G | BRN/WHT | 230 | Instrument panel lamps dimmer module output
H | GRY | 8 | Interior lamp dim signal
I | GRY/BLK | 308 | Park lamp switch output-parklamps ON
J-K | -- | -- | Not Used
L | YEL | 10 | Headlamp switch output
M | -- | -- | Not Used
N | ORN | 2340 | Fused battery feed
O | ORN | 1340 | Fused battery feed
P | LT BLU | 1872 | Park lamp switch signal-park lamps OFF
R | BRN | 9 | Park lamp feed

#### Interior Lamp and Multi-function Switch C1

Connector Part Information |

• | 12162502

• | 8-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | 650 | Ground
2 | GRY | 8 | Interior lamp dim signal
3-4 | -- | -- | Not Used
5 | DK BLU | 1393 | Courtesy lamps feed-protected battery
6-7 | -- | -- | Not Used
8 | PPL | 328 | Interior lamp override switch output

#### IP Compartment Lamp Switch

Connector Part Information |

• | 12124568

• | 2-Way M Lamp Socket Wedge Base STD (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 150 | Ground

#### LF Fog Lamp

Connector Part Information |

• | 12124819

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog lamp feed
B | BLK | 1350 | Ground

#### LF Park/Turn Lamp

Connector Part Information |

• | 12160394

• | Right Angle Type W-3 Bulb Base Sealed (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 14 | Turn signal lamp feed-left front
B | BRN | 9 | Park lamp feed
G | BLK | 1350 | Ground

#### LF Side Marker

Connector Part Information |

• | 12110053

• | Axial Type W-2 Bulb Base Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 18 | Tail/turn/stop lamp feed-left rear
B | BRN | 9 | Park lamp feed

#### LH Headlamp

Connector Part Information |

• | 12048369

• | 3-Way F Metri-Pack 280 Series Sealed (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1350 | Ground
B | TAN | 12 | Low beam headlamp feed
C | LT GRN | 11 | High beam headlamp feed

#### LH IP Courtesy Lamp

Connector Part Information |

• | 12124652

• | W2 Axial Type Lamp socket Wedge Base (CLR)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### LH License Lamp

Connector Part Information |

• | 12110053

• | Type W-2 F Axial Bulb Base (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park lamp feed
B | BLK | 450 | Ground

#### LH Roof Rail Reading Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | -- | -- | Not Used

#### LH Sunshade Lighted Vanity Mirror

Connector Part Information |

• | 12047663

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground

#### LH Taillamp

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 18 | Tail/turn/stoplamp feed - left rear
B | LT GRN/BLK | 24 | Backup lamp feed
C | -- | -- | Not Used
D | BRN | 9 | Park lamp feed
E | BLK | 350 | Ground
F | WHT | 17 | Stop lamp switch output

#### Rear Window Wiper/Washer and Multi-function Switch C3

Connector Part Information |

• | 12041301

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 1450 | Ground
C | BRN/WHT | 1571 | Traction control request input
D | BRN | 9 | Park lamp feed
E | YEL | 317 | Fog lamp relay feed-coil
F | PNK | 39 | Fused ignition 1 feed
G | PPL | 1681 | Traction control request received indicator lamp
H | PPL | 34 | Fog lamp feed

#### RF Fog Lamp

Connector Part Information |

• | 12124819

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog lamp feed
B | BLK | 1250 | Ground

#### RF Park/Turn Lamp

Connector Part Information |

• | 12160394

• | Right Angle Type W-3 Bulb Base Sealed (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 15 | Turn signal lamp feed-right front
B | BRN | 9 | Park lamp feed
G | BLK | 1250 | Ground

#### RF Side Marker

Connector Part Information |

• | 12110053

• | Axial Type W-2 Bulb Base Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
B | BRN | 9 | Park lamp feed

#### RH Headlamp

Connector Part Information |

• | 12048369

• | 3-Way F Metri-Pack 280 Series Sealed (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1250 | Ground
B | TAN | 12 | Low beam headlamp feed
C | LT GRN | 11 | High beam headlamp feed

#### RH IP Courtesy Lamp

Connector Part Information |

• | 12124652

• | 2-Way Lamp Socket Wedge Base (CLR)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### RH License Lamp

Connector Part Information |

• | 12110053

• | Type W-2 F Axial Bulb Base (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park lamp feed
B | BLK | 450 | Ground

#### RH Roof Rail Reading Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | -- | -- | Not Used

#### RH Sunshade Lighted Vanity Mirror

Connector Part Information |

• | 12047663

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground

#### RH Taillamp

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 19 | Tail/turn/stoplamp feed - right rear
B | LT GRN/BLK | 24 | Backup lamp feed
C | -- | -- | Not Used
D | BRN | 9 | Park lamp feed
E | BLK | 350 | Ground
F | WHT | 17 | Stop lamp switch output

#### RR Roof Rail Reading Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | -- | -- | Not Used

#### Stop Lamp Switch C1

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 140 | Fused battery feed
B | WHT | 17 | Stop lamp switch output

#### Windshield Header Courtesy/Reading Lamps

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | GRY/BLK | 690 | Courtesy lights control output (GND)