For 1990-2009 cars

### Removal Procedure

1. Open the sliding door.
2. Support the sliding door at the bottom.
3. Remove the pin from the sliding door center roller bracket.
4. Remove the sliding door lower roller bracket. Refer to Rear Side Door Lower Roller Bracket Replacement .
5. Remove the sliding door upper roller bracket. Refer to Rear Side Door Upper Roller Bracket Replacement .
6. With an assistant, remove the sliding door from the vehicle with the aid of an assistant.

### Installation Procedure

1. With an assistant, install the sliding door to the vehicle with the aid of an assistant.
2. Support the sliding door.
3. Install the sliding door upper roller bracket. Refer to Rear Side Door Upper Roller Bracket Replacement .
4. Install the sliding door lower roller bracket. Refer to Rear Side Door Lower Roller Bracket Replacement .
5. Install the pin to the sliding door center roller bracket.
6. Remove the support from the bottom of the sliding door.
7. Close the sliding door.