For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Headlamp and IP Lamp Dimmer Switch | Left of the instrument cluster | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control System | Lighting Systems Connector End Views in Lighting Systems
Remote Control Door Lock Receiver (RCDLR) | Behind the center of the IP, on the underside of the IP trim, near the windshield defrost vents | Keyless Entry Component Views in Keyless Entry | Keyless Entry Connector End Views in Keyless Entry
Security Indicator Lamp | Center of the IP, mounted to the trim plate, near the windshield defrost vent | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Cluster, Gauges and Console
Theft Deterrent Relay | Part of the relay center, right side of the IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control System | --
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
S202 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and rear window wiper/washer and multi-function switch breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --