For 1990-2009 cars

Causes | Correction
--- | ---
Incorrect front wheel alignment | Set the front end alignment to specification.
Contaminated brake linings | Replace the brake linings.
Incorrect tire pressure | Set the tire pressure to specification.
Loose front suspension parts | Locate and tighten/repair/replace the loose front suspension components.
Contaminated/improper brake fluid | Flush the brake system and repair the affected brake components.
Worn out brake linings | Replace the brake linings.
Uneven brake lining material | Replace the brake linings.
Glazed brake linings | Replace the brake linings.
Incorrect lining material | Replace the brake linings.
Linings damaged by abusive use | Replace the brake linings.
Scored rotor | Recondition the rotor surface or replace the rotor.
Front and/or rear brake assembly attachment loose | Locate and tighten the loose brake components.
Restricted brake fluid passage | Locate and fix the source of the brake fluid restriction.
Sticky caliper or caliper pistons | Repair/replace the caliper.
Parking brake not releasing | Malfunctioning parking brake lever or frozen parking brake cables.
Caliper to knuckle clearance | Repair as necessary.