For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Clutch Coil | Part of the A/C compressor, right side of engine at the end of the crankshaft, near the cranshaft position sensor (24x) | HVAC Component Views | HVAC Connector End Views
Auxiliary Blower Motor | Part of the auxiliary heater-A/C module, behind the left rear wheelhouse | HVAC Component Views | HVAC Connector End Views
Auxiliary Blower Motor Resistor | Part of the auxiliary heater-A/C module, rear of the auxiliary blower motor | HVAC Component Views | HVAC Connector End Views
Auxiliary Coolant Bypass Pump | Engine Compartment above the air cleaner assembly secured to the diagonal brace bracket | HVAC Component Views | HVAC Connector End Views
Auxiliary Coolant Pump Switch | Body front, inside center front bumper beam | HVAC Component Views | HVAC Connector End Views
Auxiliary Heater-A/C Control (Auxiliary Blower Switch) (4 Door) | Part of the left rear armrest | HVAC Component Views | HVAC Connector End Views
Auxiliary Heater-A/C Control (Temperature Control) (4 Door) | Part of the left rear armrest | HVAC Component Views | HVAC Connector End Views
Auxiliary Heater-A/C Control (Auxiliary Blower Switch) (5 Door) | Part of the rear roof console, behind the driver seat | HVAC Component Views | HVAC Connector End Views
Auxiliary Heater-A/C Control (Temperature Control) (5 Door) | Part of the rear roof console, behind the driver seat | HVAC Component Views | HVAC Connector End Views
Auxiliary Temperature Valve Actuator | Part of the auxiliary heater-A/C module, below the auxiliary blower motor | HVAC Component Views | HVAC Connector End Views
Blower Motor | Part of the heater-A/C module, behind the right side of the IP compartment | HVAC Component Views | --
Blower Motor Resistor | Part of the heater-A/C module, behind the right side of the IP compartment, in front of the blower motor | HVAC Component Views | HVAC Connector End Views
Electric Air Inlet Actuator | Right side of the IP, above the blower motor, near the relay center, and the BCM | HVAC Component Views | HVAC Connector End Views
Electric Slave Actuator | Left side of the heater-A/C module, left of the radio above the knee bolster | HVAC Component Views | HVAC Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Heater-A/C Control | Center of the IP, below the radio | HVAC Component Views | HVAC Connector End Views
Heater-A/C Control (Blower Motor Switch) | Part of the heater-A/C control | HVAC Component Views | HVAC Connector End Views
Heater-A/C Control (Compressor and Air Delivery Control) | Part of the heater-A/C control | HVAC Component Views | HVAC Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Rear Window Wiper/Washer and Multi-function Switch | Center of the IP, below the radio | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Window Wiper/Washer and Multi-function Switch (Auxiliary Blower Switch) | Part of the rear window wiper/washer and multi-function switch | Wiper/Washer Component Views | HVAC Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
G117 | Engine compartment, left and above the starter, near the starter solenoid | Harness Routing Views | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
G301 | Secured to the inside of the lower left B-pillar | Harness Routing Views | --
G401 | Secured to the lower left D-pillar | -- | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
S105 | Engine harness, top right side radiator approximately 20 cm (8 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S202 | IP harness, leftt side of the IP approximately 15 cm (6 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S213 | IP harness, center of IP approximately 72 cm (28 in) from the cigar lighter | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S252 | IP harness, center of the IP approximately 76 cm (30 in) from the cigar lighter | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S339 | Body harness, front of the left B-pillar approximately 26 cm (10 in) from the G301 breakout | -- | --
S341 | Body harness, in front of the left wheelhouse approximately 13 cm (5 in) from the radio rear speaker amplifier breakout | -- | --
S343 | Body harness, in front of the left wheelhouse approximately 40 cm (16 in) from the radio rear speaker amplifier breakout | -- | --
S345 | Body harness, in front of the left rear wheelhouse approximately 48 cm (19 in) from the left sliding door jamb switch | -- | --
S403 | Body harness, left rear of the body on top of the wheel well approximately 13 cm (5 in) from the top and rear clips | -- | --