For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
2. Remove the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.
3. Remove the right instrument panel courtesy lamp from the instrument panel.
4. Remove the left instrument panel courtesy lamp from the instrument panel.

### Installation Procedure

1. Install the right instrument panel courtesy lamp to the instrument panel insulator.
2. Install the left instrument panel courtesy lamp to the instrument panel insulator.
3. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
4. Install the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.