For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Quarter Wheel Opening Molding Screw | 2 N·m | 18 lb in
Grille Center Bolts | 4 N·m | 35 lb in
Lower Front Quarter Wheel Opening Molding Screw | 2 N·m | 18 lb in
Lower Quarter Wheel Opening Molding Retainer Nut | 2 N·m | 18 lb in
Lower Rear Fender Wheel Opening Molding Screw | 2 N·m | 18 lb in
Rear Rocker Molding Retainer Nut | 2 N·m | 18 lb in
Rear Quarter Molding Screw | 2 N·m | 18 lb in