For 1990-2009 cars

Table 1: | Air Inflator Switch
Table 2: | Auto Level Control (ALC) Air Compressor (With Inflator)
Table 3: | Auto Level Control (ALC) Air Compressor (Without Inflator)
Table 4: | Auto Level Control (ALC) Air Inflator Relay
Table 5: | Auto Level Control (ALC) Air Inflator Solenoid Valve
Table 6: | Auto Level Control (ALC) Sensor (With Inflator)
Table 7: | Auto Level Control (ALC) Sensor (Without Inflator)

#### Air Inflator Switch

Connector Part Information |

• | 1201-5683

• | 3-Way F Pin Grip Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 1245 | Auto Level Control Inflator Switch Output
B | BLK | 1725 | Ground
C | PPL | 1267 | Auto Level Control Reset Signal

#### Auto Level Control (ALC) Air Compressor (With Inflator)

Connector Part Information |

• | 1205-9472

• | 7-Way F Metri-Pack Mixed Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 743 | Ignition 2 Feed
B | WHT | 320 | Auto Level Control Air Compressor Vent Solenoid Output
C | ORN | 1240 | Fused Battery Feed
D | YEL | 321 | Auto Level Control Compressor Relay Output-Coil
E | ORN | 1240 | Fused Battery Feed
F | -- | -- | Not Used
G | BLK | 1725 | Ground

#### Auto Level Control (ALC) Air Compressor (Without Inflator)

Connector Part Information |

• | 1205-9472

• | 7-Way F Metri-Pack Mixed Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 743 | Fused Ignition 2 Feed
B | WHT | 320 | Auto Level Control Air Compressor Vent Solenoid Output
C | ORN | 1240 | Fused Battery Feed
D | YEL | 321 | Auto Level Control Compressor Relay Output-Coil
E | ORN | 1240 | Fused Battery Feed
F | -- | -- | Not Used
G | BLK | 1725 | Ground

#### Auto Level Control (ALC) Air Inflator Relay

Connector Part Information |

• | 0296-5977

• | 8-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1267 | Auto Level Control Reset Signal
B | LT BLU | 1248 | Auto Level Control Power Output
C | DK BLU | 1249 | Auto Level Control Solenoid Valve Feed
D | ORN | 1240 | Fused Battery Feed
E | YEL | 321 | Auto Level Control Compressor Relay Output-Coil
F | WHT | 1245 | Auto Level Control Inflator Switch Output
G | -- | -- | Not Used
H | BLK | 1725 | Ground

#### Auto Level Control (ALC) Air Inflator Solenoid Valve

Connector Part Information |

• | 0298-4951

• | 2-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1725 | Ground
B | DK BLU | 1249 | Battery Fused Feed

#### Auto Level Control (ALC) Sensor (With Inflator)

Connector Part Information |

• | 1205-2848

• | 6-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1725 | Ground
B | YEL | 321 | Auto Level Control Compressor Relay Output-Coil
C | LT BLU | 1248 | Auto Level Control Power Input
D | YEL | 743 | Fused Ignition 2 Feed
E | WHT | 320 | Auto Level Control Air Compressor Vent Solenoid Output
F | -- | -- | Not Used

#### Auto Level Control (ALC) Sensor (Without Inflator)

Connector Part Information |

• | 1205-2848

• | 6-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1725 | Ground
B | YEL | 321 | Auto Level Control Compressor Relay Output-Coil
C | ORN | 1240 | Fused Battery Feed
D | YEL | 743 | Fused Ignition 2 Feed
E | WHT | 320 | Auto Level Control Air Compressor Vent Solenoid Output
F | -- | -- | Not Used