For 1990-2009 cars

## Dimensions - Body Long Wheelbase

Reference Number | Length | Width | Height | Feature Size
--- | --- | --- | --- | ---
1 | 449 | 781 | 1113 | 15 mm front hinge gage hole
2 | 415 | 805 | 734 | 18x15 mm front hinge gage hole
3 | 730 | 831 | 1022 | 18 mm door stricker
4 | 2799 | 418 | 1794 | hinge mounting
5 | 2795 | 140 | 1791 | Wire access hole
6 | 3138 | 20 | 745 | Wire access hole
7 | 3112 | 509 | 667 | 17 mm bumper attachment hole
8 | 3112 | 355 | 562 | 17 mm bumper attachment hole
9 | 3112 | 509 | 562 | 17 mm bumper attachment hole
10 | 2999 | 809 | 957 | Taillamp attachment
All dimensions are measured from a zero line, center line, and a common datum. All dimensions are symmetrical unless otherwise specified.

## Dimensions - Body Short Wheelbase

Reference Number | Length | Width | Height | Feature Size
--- | --- | --- | --- | ---
1 | 449 | 781 | 1113 | 15 mm front hinge gage hole
2 | 415 | 805 | 734 | 18x15 mm front hinge gage slot
3 | 730 | 831 | 1022 | 18 mm Door lock stricker
4 | 2444 | 418 | 1781 | Hinge mounting
5 | 2440 | 140 | 1778 | Wire access hole
6 | 2784 | 20 | 731 | 15 mm lock stricker attachment hole
7 | 2757 | 509 | 654 | 17 mm bumper attachment hole
8 | 2757 | 355 | 549 | 17 mm bumper attachment hole
9 | 2757 | 509 | 549 | 17 mm bumper attachment hole
10 | 2644 | 809 | 945 | Taillamp Attachment
All dimensions are measured from a zero line, center line, and a common datum. All dimensions are symmetrical unless otherwise specified.

## Dimensions - Body Engine Compartment

Reference Number | Length | Width | Height | Feature Size
--- | --- | --- | --- | ---
1 | 950 | 687 | 1028 | 11 mm diagonal brace hole
2 | 1516 | 279 | 920 | 7 mm diagonal brace hole
3 | 1483 | 304 | 930 | 7 mm diagonal brace hole
4 | 1525 | 357 | 918 | Head liner panel mounting
5 | 1372 | 626 | 1021 | Head liner panel mounting
6 | 1549 | 617 | 675 | Bumper attachment
7 | 1549 | 617 | 606 | 8½x15 mm bumper attachment slot
8 | 1585 | 450 | 606 | Bumper attachment
9 | 1585 | 450 | 675 | bumper atachment
All dimensions are measured from a zero line, center line, and a common datum. All dimensions are symmetrical unless otherwise specified.

## Dimensions - Body Body Side

Reference Number | Length | Width | Height | Feature Size
--- | --- | --- | --- | ---
1 | 1816 | 817 | 1132 | 18 mm door lock striker hole
2 | 669 | 813 | 1033 | 18 mm door lock striker hole
3 | 449 | 781 | 1113 | 15 mm front hinge gage hole
4 | 415 | 805 | 734 | 18x15 mm front hinge gage hole
5 | 702 | 756 | 1180 | 12 mm hood attachment hole
6 | 814 | 756 | 1180 | 12 mm hood attachment hole
7 | 875 | 750 | 1169 | 5 mm fender attachment hole
8 | 1113 | 732 | 1100 | 5 mm fender attachment hole
9 | 1331 | 716 | 1037 | 5 mm fender attachment hole
10 | 1370 | 713 | 1026 | 5 mm fender attachment hole
All dimensions are measured from a zero line, center line, and a common datum. All dimensions are symmetrical unless otherwise specified.