For 1990-2009 cars

Reference Number | Length | Width | Height | Feature Size
--- | --- | --- | --- | ---
1 | 1433 | 542 | 584 | 30x19 gage slot
2 | 1500 | 530 | 586 | Cradle mounting hole
3 | 480 | 270 | 420 | 60 mm cradle gage hole
4 | 480 | 259 | 420 | 20x27 mm cradle gage hole
5 | - | 432 | 423 | 20 mm flanged gage hole
6 | 412 | 205 | 396 | 12 mm hole
7 | 1463 | 432 | 529 | 20 mm flanged gage hole
8 | 2407 | 432 | 580 | 20 mm flanged gage slot
9 | 2909 | 432 | 587 | Exhaust mounting (LWB)
All dimensions are measured from a zero line, a center line and common datum. All dimensions are symmetrical unless otherwise specificed.