For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Cruise Control Module | Engine compartment, near the left strut tower | Cruise Control Component Views | Cruise Control Connector End Views
Cruise Control Release Switch | Mounted to the brake pedal support | Cruise Control Component Views | Cruise Control Connector End Views
Cruise Control Switch | Part of the turn signal switch, on the turn signal lever | Theft Deterrent System Component Views | Cruise Control Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Stop Lamp Switch | Mounted to the brake pedal support | Cruise Control Component Views | Lighting Systems Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views | Inline Harness Connector End Views
G201 | Left side of the IP, secured on the underside of the cross car beam, above the park brake assembly | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
S205 | IP harness, left side of the IP approximately 8 cm (3 in) from the hazard lamp/turn signal flasher breakout | -- | --
S266 | IP harness, left side of the IP approximately 24 cm (9 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --