For 1990-2009 cars

### Removal Procedure

1. Remove the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument panel, Gages and Console.
2. Remove the theft deterrent relay (1) from the relay block.

### Installation Procedure

1. Install the theft deterrent relay (1) to the relay block.
2. Install the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.