For 1990-2009 cars

Figure 1: |

#### Emission Hose Routing

(1) | To Rocker Arm Cover
(2) | EVAP Service Port
(3) | To EVAP Canister (At Rear of Vehicle)
(4) | Air Intake Duct
(5) | Throttle Body
(6) | PCV Valve
(7) | Fuel Pressure Regulator
(8) | To Transaxle
(9) | Intake Manifold
(10) | To Accessory
(11) | To Vacuum Brake Booster
(12) | MAP Sensor
(13) | EVAP Canister Purge Valve

Figure 2: |

#### EVAP Control System Overview

(1) | EAVP Vent Valve/Solenoid
(2) | EVAP Vent Valve/Solenoid Ignition Feed Circuit Terminal
(3) | EVAP Vent Valve/Solenoid Control Circuit Terminal
(4) | EVAP Vent Valve/Solenoid Filter
(5) | EVAP Vapor Lines
(6) | Fuel Tank Pressure Sensor
(7) | Fuel Tank Pressure Sensor Ground Circuit Terminal
(8) | Fuel Tank Pressure Sensor Signal Circuit Terminal
(9) | Fuel Tank Pressure Sensor Circuit 5 Volt Reference Circuit Terminal
(10) | Fuel Filler Pipe
(11) | Modular Fuel Sender Assembly
(12) | Fuel Limiter Vent Valve (FLVV)
(13) | Pressure/Vacuum Relief Valve (Optional)
(14) | EVAP Canister
(15) | EVAP Canister Purge Valve/Solenoid Ignition Feed Circuit Terminal
(16) | EVAP Canister Purge Valve/Solenoid Control Circuit Terminal
(17) | Intake Manifold Vacuum Source
(18) | EVAP Canister Purge Valve/Solenoid
(19) | EVAP Service Port