For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Refer to Caution: When you are performing service on or near the SIR components or the SIR wiring, you must disable the SIR system. Refer to Disabling the SIR System. Failure to follow the correct procedure could cause air bag deployment, personal injury, or unnecessary SIR system repairs. in Cautions and Notices.
| In order to prevent accidental deployment, the shorting bars close in order to short the connectors when the connectors are separated.