For 1990-2009 cars

The flexible hydraulic brake hoses transmit hydraulic pressure from the steel brake lines on the body to the calipers. Inspect the hoses at least twice a year.

Inspect the hoses for the following conditions:

• | Road hazard damage

• | Cracks

• | Chafing of the outer cover

• | Leaks

• | Blisters

• | Proper routing and mounting

Use a light and mirror for an adequate inspection. Replace any brake hoses with any of the above conditions.