For 1990-2009 cars

Table 1: | IPC Scan Tool Data List
Table 2: | EBCM Scan Tool Data List

The IPC and the EBCM Scan Tool Data Lists contain all the antilock brake system related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The column, 'Data List,' indicates the location of the parameter within the scan tool menu selections.

Use the IPC and the EBCM Scan Tool Data Lists as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all the diagnostic procedures with the ABS Diagnostic Starting Point. Use the IPC and the EBCM Scan Tool Data Lists only after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

| OR

• | The DTC or symptom diagnostic procedure indicated by the diagnostic system check does not resolve the customer concern.

The Typical Data Values are obtained from a properly operating vehicle under the conditions specified in the first row of the Scan Tool Data List table. Comparison of the parameter values from the suspect vehicle with the Typical Data Values may reveal the source of the customer concern.

The ID Information menu is located on the EBCM main screen.

#### IPC Scan Tool Data List

Ignition is ON, engine OFF, and vehicle is stationary
Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition 1 | Data Display | Volts | B+

#### EBCM Scan Tool Data List

Ignition is ON, engine OFF, and vehicle is stationary
Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
ABS Active | Data Display | Yes/No | No
ABS Relay Command | Data Display | On/Off | On
ABS Relay Feedback | Data Display | On/Off | On
ABS Warning Lamp | Data Display | On/Off | Off
Brake Fluid Level | Data Display | Low/OK | OK
Brake Switch Status | Data Display | Applied/Released | Released
Brake Temp Status | Data Display | Normal/Over Temp | Normal
Configuration ID | ID Information | Numeric | varies
DE Base Part Number | ID Information | Numeric | varies
DE Build Sequence Number | ID Information | Numeric | varies
DE Calibration Part Number | ID Information | Numeric | varies
DE End Model Part Number | ID Information | Numeric | varies
DE ROM Part Number | ID Information | Numeric | varies
EBCM to PCM Requested Torque | Data Display | % | 90
Ignition Voltage | Data Display | Volts | B+
Julian Date Code | ID Information | Numeric | varies
Left Front Wheel Speed | Data Display | km/h or mph | 0
Left Rear Wheel Speed | Data Display | km/h or mph | 0
LF Inlet Valve Solenoid | Data Display | Active/Inactive | Inactive
LF Outlet Valve Solenoid | Data Display | Active/Inactive | Inactive
LF Rotor Temperature | Data Display | °C/°F | varies
LR Inlet Valve Solenoid | Data Display | Active/Inactive | Inactive
LR Outlet Valve Solenoid | Data Display | Active/Inactive | Inactive
PCM to EBCM Delivered Torque | Data Display | % | 10
Pump Motor Commanded State | Data Display | On/Off | Off
Pump Motor Feedback State | Data Display | On/Off | Off
RF Inlet Valve Solenoid | Data Display | Active/Inactive | Inactive
RF Outlet Valve Solenoid | Data Display | Active/Inactive | Inactive
RF Rotor Temperature | Data Display | °C/°F | varies
Right Front Wheel Speed | Data Display | km/h or mph | 0
Right Rear Wheel Speed | Data Display | km/h or mph | 0
Rough Road Parameter | Data Display | g | 0.00
RR Inlet Valve Solenoid | Data Display | Active/Inactive | Inactive
RR Outlet Valve Solenoid | Data Display | Active/Inactive | Inactive
Switched Battery Voltage | Data Display | Volts | B+
System ID | ID Information | Numeric | varies
TCS Active | Data Display | Yes/No | No
TCS Active Lamp | Data Display | On/Off | Off
TCS Disable Lamp | Data Display | On/Off | Off
TCS Enable Status | Data Display | Enable/Disable | Disable
TCS Equipped | ID Information | Yes/No | Yes or No
TCS Failed | Data Display | Yes/No | No
TCS Warning Lamp | Data Display | On/Off | Off
Vehicle Speed | Data Display | km/h or mph | 0