For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views | Body Control System Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Retained Accessory Power Relay | In the relay center | Power and Grounding Component Views | Power and Grounding Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S227 | Video entertainment harness behind right side of hush panel | -- | --
S263 | IP harness, right side of the IP at the electric air inlet actuator breakout | -- | --