For 1990-2009 cars

Table 1: | Door Lock Switch Plate (Door Mounted, Plunger)
Table 2: | Front Door Lock Connector C1 (Ajar Indicator Switch)
Table 3: | Front Door Lock Connector C2 (Actuator)
Table 4: | Front Door Lock Cylinder Switch
Table 5: | Front Door Lock Switch
Table 6: | Front Window Regulator Motor
Table 7: | Interior Lamp and Multi-function Switch Connector C3 (Power Sliding Door On/Off Switch and Power Sliding Door Open/Close Switch)
Table 8: | Interior Lamp and Multi-function Switch Connector C4 (Rear Quarter Window Switch)
Table 9: | LH Door Lock Switch Plate (Pillar Mounted, Striker)
Table 10: | LF Window Switch
Table 11: | Outside Rearview Mirror (Mirror Motor Pack and Heated Defogger)
Table 12: | Outside Rearview Mirror Remote Control Switch
Table 13: | Power Sliding Door Detent Switch
Table 14: | Power Sliding Door Open/Close Switch (RH B-Pillar)
Table 15: | Power Sliding Door Unlatch Actuator
Table 16: | Rear Door Lock (Actuator)
Table 17: | Rear Quarter Window Actuator
Table 18: | Rear Side Door Actuator Control Module Connector C1
Table 19: | Rear Side Door Actuator Control Module Connector C2
Table 20: | Rear Side Door Actuator Control Module Connector C3
Table 21: | Rear Side Door Actuator Control Module Connector C4
Table 22: | Rear Side Door Actuator Control Module C5
Table 23: | RF Window Switch
Table 24: | RH Door Lock Switch Plate (Pillar Mounted, Striker)
Table 25: | Sliding Door Jamb Switch

#### Door Lock Switch Plate (Door Mounted, Plunger)

Connector Part Information |

• | 1216-0716

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Passenger Door Lock Actuator Feed
B | TAN | 294 | Passenger Door Unlock Actuator Feed
C | BLK | 750 | Ground (RH +E58)
D | BLK | 750 | Ground (RH +E58)
E | YEL | 1892 | Power Sliding Door Detent Switch Input (RH +E58)
F | YEL | 1892 | Power Sliding Door Detent Switch Input (RH +E58)
G | GRY | 295 | Power Sliding Door Unlatch Actuator Feed (RH +E58)
H | -- | -- | Not Used

#### Front Door Lock Connector C1 (Ajar Indicator Switch)

Connector Part Information |

• | 1216-2190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 159 | Key In Ignition Output (LH)
A | BLK | 750 | Ground (RH)
B | YEL | 804 | Door Ajar Indicator Lamp Output (LH)
C | YEL | 804 | Door Ajar Indicator Lamp Output (RH)
D | BLK | 750 | Ground (LH)
D | DK BLU | 49 | Driver Door Switch Signal (RH)

#### Front Door Lock Connector C2 (Actuator)

Connector Part Information |

• | 1530-0027

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Door Unlock Motor Feed
B | GRY | 295 | Door Lock Motor Feed

#### Front Door Lock Cylinder Switch

Connector Part Information |

• | 1212-4583

• | 4-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLK | 780 | Key Cylinder Door Lock Output
B | -- | -- | Not Used
C | BLK | 750 | Ground
D | ORN/BLK | 781 | Key Cylinder Door Unlock Output

#### Front Door Lock Switch

Connector Part Information |

• | 1208-9527

• | 6-Way F Metri-Pack 280 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 195 | Door Lock Switch Input Feed
B | BLK | 750 | Ground
C | GRY | 8 | Interior Lamps Dimming Input Feed
D | WHT | 194 | Door Unlock Switch Input Feed
E | BLK | 750 | Ground
F | -- | -- | Not Used

#### Front Window Regulator Motor

Connector Part Information |

• | 1212-9487

• | 2-Way F Metri-Pack 280 Series Flexlock (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 164 | Power Window Up Direction Motor Feed (LH)
A | DK BLU | 666 | Power Window Up Direction Motor Feed (RH)
B | BRN | 165 | Power Window Down Direction Motor Feed (LH)
B | BRN | 667 | Power Window Down Direction Motor Feed (RH)

#### Interior Lamp and Multi-function Switch Connector C3 (Power Sliding Door On/Off Switch and Power Sliding Door Open/Close Switch)

Connector Part Information |

• | 1204-1301

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior Lamps Dimming Input Feed
B | BLK | 650 | Ground
C | LT BLU | 1894 | Power Sliding Door Open/Close Output
D | BLK/WHT | 1896 | Power Sliding Door On/Off Output
E-H | -- | -- | Not Used

#### Interior Lamp and Multi-function Switch Connector C4 (Rear Quarter Window Switch)

Connector Part Information |

• | 1204-7976

• | 8-Way F Metri-Pack 280 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior Lamps Dimming Input Feed
B | BLK | 650 | Ground
C | BRN | 902 | Rear Quarter Window Open Output Feed
D | BLK | 901 | Rear Quarter Window Close Output Feed
E | YEL | 743 | Fused Input Feed
F-H | -- | -- | Not Used

#### LH Door Lock Switch Plate (Pillar Mounted, Striker)

Connector Part Information |

• | 1216-0716

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Passenger Door Lock Actuator Feed
B | TAN | 294 | Passenger Door Unlock Actuator Feed
C-H | -- | -- | Not Used

#### LF Window Switch

Connector Part Information |

• | 1206-4998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 165 | Power Window Down Direction Motor Feed
B | LT BLU | 166 | RF Window Switch Up Direction Feed
C | -- | -- | Not Used
D | GRY | 8 | Interior Lamps Dimming Input Feed
E | DK BLU | 164 | Power Window Up Direction Motor Feed
F | TAN | 167 | RF Window Switch Down Direction Feed
G | BLK | 750 | Ground
H | BRN | 143 | Fused Input Feed

#### Outside Rearview Mirror (Mirror Motor Pack and Heated Defogger)

Connector Part Information |

• | 1206-5781

• | 6-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 81 | Power Mirror Left/Right Motor Feed (LH)
A | RED/WHT | 881 | Power Mirror Left/Right Motor Feed (RH)
B | LT GRN | 1499 | Power Mirror Select Switch Feed (Left)
B | LT BLU/WHT | 1497 | Power Mirror Select Switch Feed (Right)
C | YEL | 88 | Power Mirror Up/Down Motor Feed (LH)
C | BRN/WHT | 1498 | Power Mirror Up/Down Motor Feed (RH)
D | -- | -- | Not Used
E | ORN | 267 | Heated Mirror Feed
F | BLK | 750 | Ground

#### Outside Rearview Mirror Remote Control Switch

Connector Part Information |

• | 1204-7886

• | 8-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 1498 | RH Outside Rearview Mirror Up/Down Output Feed
B | RED/WHT | 881 | RH Outside Rearview Mirror Right/Left Output Feed
C | LT BLU/WHT | 1497 | RH Outside Rearview Mirror Motor Ground Feed
D | BLK | 750 | Ground
E | ORN | 1140 | Fused Input Feed
F | WHT | 81 | LH Outside Rearview Mirror Motor Right/Left Output Feed
G | YEL | 88 | LH Outside Rearview Mirror Motor Up/Down Output Feed
H | LT GRN | 1499 | LH Outside Rearview Mirror Motor Ground Feed

#### Power Sliding Door Detent Switch

Connector Part Information |

• | 1205-2642

• | 2-Way F Metri-Pack 150 Series Sealed (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 1892 | Detent Switch Output
B | BLK | 750 | Ground

#### Power Sliding Door Open/Close Switch (RH B-Pillar)

Connector Part Information |

• | 1206-4860

• | 6-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 1894 | Power Sliding Door Open/Close Output Feed
B | GRY | 8 | Interior Lamps Dimming Input Feed
C | -- | -- | Not Used
D | BLK | 650 | Ground
E | BLK | 650 | Ground
F | -- | -- | Not Used

#### Power Sliding Door Unlatch Actuator

Connector Part Information |

• | 1207-7900

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 750 | Ground
B | BLK | 2910 | Power Sliding Door Release Actuator Control Input

#### Rear Door Lock (Actuator)

Connector Part Information |

• | 1207-7900

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Door Lock Motor Feed
B | TAN | 294 | Door Unlock Motor Feed

#### Rear Quarter Window Actuator

Connector Part Information |

• | 1205-2832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 901 | Rear Quarter Window Close Input Feed
B | BRN | 902 | Rear Quarter Window Open Input Feed

#### Rear Side Door Actuator Control Module Connector C1

Connector Part Information |

• | 1204-1429

• | 5-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | ORN | 340 | Fused Input Feed
D | BLK | 2910 | Power Sliding Door Release Actuator Control
E | BLK | 1850 | Ground

#### Rear Side Door Actuator Control Module Connector C2

Connector Part Information |

• | 1206-6130

• | 9-Way F Micro-Pack 100 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | -- | -- | Not Used
8 | DK GRN | 389 | Vehicle Speed Signal Input
9 | YEL | 1892 | Detent Switch Input
10 | LT BLU | 1894 | Power Sliding Door Open/Close Input
11 | PNK | 39 | Fused Input Feed
12 | ORN | 640 | Fused Input Feed
13 | BLK/WHT | 1896 | Power Sliding Door On/Off Input
14 | LT GRN | 275 | Transaxle Park Position Safety Input
15 | -- | -- | Not Used

#### Rear Side Door Actuator Control Module Connector C3

Connector Part Information | 4-Way Connector (BLK)
--- | ---
Pin | Wire Color | Circuit No. | Function
A | BLK | 902 | Power Sliding Door Alarm Switch to B+ Output Feed
B | WHT | 901 | Power Sliding Door Alarm Ground
C | BRN | -- | Clutch Control High Feed
D | DK GRN | -- | Clutch Control Low Feed

#### Rear Side Door Actuator Control Module Connector C4

Connector Part Information | 2-Way Connector (BLK)
--- | ---
Pin | Wire Color | Circuit No. | Function
A | RED | -- | Cable Motor Control Return
B | GRN | -- | Cable Motor Control Power

#### Rear Side Door Actuator Control Module C5

Connector Part Information | 4-Way Connector (WHT)
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK | -- | Optical Sensor Input/Output
2 | BLK | -- | Optical Sensor Input/Output
3 | BLK | -- | Optical Sensor Input/Output
4 | BLK/WHT | -- | Optical Sensor Input/Output

#### RF Window Switch

Connector Part Information |

• | 1206-4998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 666 | Power Window Up Direction Motor Feed
B | GRY | 8 | Interior Lamps Dimming Input Feed
C | BLK | 750 | Ground
D | TAN | 167 | RF Window Switch Down Direction Feed
E | BRN | 667 | Power Window Down Direction Motor Feed
F | BRN | 141 | Fused Input Feed
G | -- | -- | Not Used
H | LT BLU | 166 | RF Window Switch Up Direction Feed

#### RH Door Lock Switch Plate (Pillar Mounted, Striker)

Connector Part Information |

• | 1216-0716

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Passenger Door Lock Actuator Feed
B | TAN | 294 | Passenger Door Unlock Actuator Feed
C | BLK | 750 | Ground (+E58)
D | BLK | 750 | Ground (+E58)
E | YEL | 1892 | Power Sliding Door Detent Switch Input (+E58)
F | YEL | 1892 | Power Sliding Door Detent Switch Input (+E58)
G | BLK | 2910 | Power Sliding Door Release Actuator Input (+E58)
H | -- | -- | Not Used

#### Sliding Door Jamb Switch

Connector Part Information |

• | 1206-5422

• | 3-Way F Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 804 | Door Ajar Indicator Lamp Output
B | ORN | 54 | Passenger Door Switch Signal
C | BLK | 750 | Ground